| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Memory To Memory Definitions
BLUENRG1 Peripheral Driver » DMA Peripheral » Exported Constants

## Macros

#define | DMA_M2M_Enable ((uint32_t)0x00004000)
#define | DMA_M2M_Disable ((uint32_t)0x00000000)
#define | IS_DMA_M2M_STATE(STATE) (((STATE) == DMA_M2M_Enable) || ((STATE) == DMA_M2M_Disable))

## Detailed Description

## Macro Definition Documentation

#define DMA_M2M_Disable ((uint32_t)0x00000000)

Definition at line 191 of file BlueNRG1_dma.h.

#define DMA_M2M_Enable ((uint32_t)0x00004000)

Definition at line 190 of file BlueNRG1_dma.h.

#define IS_DMA_M2M_STATE | ( |  | STATE | ) | (((STATE) == DMA_M2M_Enable) || ((STATE) == DMA_M2M_Disable))

Definition at line 192 of file BlueNRG1_dma.h.