| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Memory Incremented Mode Definitions
BLUENRG1 Peripheral Driver » DMA Peripheral » Exported Constants

## Macros

#define | DMA_MemoryInc_Enable ((uint32_t)0x00000080)
#define | DMA_MemoryInc_Disable ((uint32_t)0x00000000)
#define | IS_DMA_MEMORY_INC_STATE(STATE)

## Detailed Description

## Macro Definition Documentation

#define DMA_MemoryInc_Disable ((uint32_t)0x00000000)

Definition at line 124 of file BlueNRG1_dma.h.

#define DMA_MemoryInc_Enable ((uint32_t)0x00000080)

Definition at line 123 of file BlueNRG1_dma.h.

#define IS_DMA_MEMORY_INC_STATE | ( |  | STATE | ) |

Value:
(((STATE) == DMA_MemoryInc_Enable) || \
((STATE) == DMA_MemoryInc_Disable))
DMA_MemoryInc_Disable
#define DMA_MemoryInc_Disable
Definition: BlueNRG1_dma.h:124
DMA_MemoryInc_Enable
#define DMA_MemoryInc_Enable
Definition: BlueNRG1_dma.h:123

Definition at line 125 of file BlueNRG1_dma.h.