| BlueNRG-1 Peripherals drivers Examples

- Main Page
- Modules
- Classes
- Files

Macros | Functions
GPIO Wake-up Example
BlueNRG1 Standard Peripheral Examples » GPIO Examples

## Macros

#define | SYST_CLOCK 16000000 /* System clock frequency */

## Functions

void | SWDClk_Interrupt_Configuration (void)
| GPIO Interrupt Configuration. Configure interrupt on rising edge on SWD_CLK_PIN. More...
int | main (void)
| Main program code. More...

## Detailed Description

## Macro Definition Documentation

#define SYST_CLOCK 16000000 /* System clock frequency */

Definition at line 176 of file GPIO_IOWakeup_main.c.

## Function Documentation

int main | ( | void |  | ) |

Main program code.

Parameters

  None |

Return values

  None |

Definition at line 191 of file GPIO_IOWakeup_main.c.

void SWDClk_Interrupt_Configuration | ( | void |  | ) |

GPIO Interrupt Configuration. Configure interrupt on rising edge on SWD_CLK_PIN.

Parameters

  None |

Return values

  None |

Definition at line 231 of file GPIO_IOWakeup_main.c.