| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Data Transfer Direction Definitions
BLUENRG1 Peripheral Driver » DMA Peripheral » Exported Constants

## Macros

#define | DMA_DIR_PeripheralDST ((uint32_t)0x00000010)
#define | DMA_DIR_PeripheralSRC ((uint32_t)0x00000000)
#define | IS_DMA_DIR(DIR)

## Detailed Description

## Macro Definition Documentation

#define DMA_DIR_PeripheralDST ((uint32_t)0x00000010)

Definition at line 99 of file BlueNRG1_dma.h.

#define DMA_DIR_PeripheralSRC ((uint32_t)0x00000000)

Definition at line 100 of file BlueNRG1_dma.h.

#define IS_DMA_DIR | ( |  | DIR | ) |

Value:
(((DIR) == DMA_DIR_PeripheralDST) || \
((DIR) == DMA_DIR_PeripheralSRC))
DMA_DIR_PeripheralDST
#define DMA_DIR_PeripheralDST
Definition: BlueNRG1_dma.h:99
DMA_DIR_PeripheralSRC
#define DMA_DIR_PeripheralSRC
Definition: BlueNRG1_dma.h:100

Definition at line 101 of file BlueNRG1_dma.h.