| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

Functions | Variables
SDK_EVAL_Config.c File Reference

This file provides all the low level API to manage SDK Version identification. More...

`#include "BlueNRG1.h"`
`#include "BlueNRG1_conf.h"`
`#include "SDK_EVAL_Config.h"`

Go to the source code of this file.

## Functions

void | SdkEvalIdentification (void)
| Identify the version of the current BlueNRG1 platform. More...
uint8_t | SdkEvalGetVersion (void)
| Returns the version of the current BlueNRG1 platform. More...

## Variables

const uint32_t | s_vectnButtonPinVersion [SDK_PLATFORMS_NUMBER][EVAL_BOARD_BUTTONS] = {{GPIO_Pin_13, GPIO_Pin_5}}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) Buttons definitions. More...
const uint32_t | s_UartTxPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_8}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) UART definitions. More...
const uint32_t | s_UartTxModeVersion [SDK_PLATFORMS_NUMBER] = {Serial1_Mode}
const uint32_t | s_UartRxPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_11}
const uint32_t | s_UartRxModeVersion [SDK_PLATFORMS_NUMBER] = {Serial1_Mode}
const I2C_Type * | s_I2cPeripheralVersion [SDK_PLATFORMS_NUMBER] = {I2C2}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) I2C definitions. More...
const uint32_t | s_I2cDataPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_5}
const uint32_t | s_I2cDataModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_I2cClkPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_4}
const uint32_t | s_I2cClkPinModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const DMA_CH_Type * | s_I2cDataDmaTxVersion [SDK_PLATFORMS_NUMBER] = {DMA_CH7}
const uint32_t | s_I2cDataDmaRxTcVersion [SDK_PLATFORMS_NUMBER] = {DMA_FLAG_TC6}
const DMA_CH_Type * | s_I2cDataDmaRxVersion [SDK_PLATFORMS_NUMBER] = {DMA_CH6}
const uint32_t | s_I2cDataDmaTxTcVersion [SDK_PLATFORMS_NUMBER] = {DMA_FLAG_TC7}
const uint32_t | s_I2CBaseVersion [SDK_PLATFORMS_NUMBER] = {I2C2_BASE}
const uint32_t | s_vectnGpioPinVersion [SDK_PLATFORMS_NUMBER][EVAL_BOARD_LEDS] = {{GPIO_Pin_6, GPIO_Pin_7, GPIO_Pin_14}}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) LEDs definitions. More...
const uint32_t | s_SpiCs1PinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_1}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) SPI definitions. More...
const uint32_t | s_SpiCs1ModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiCs2PinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_11}
const uint32_t | s_SpiCs2ModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiMosiPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_2}
const uint32_t | s_SpiMosiModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiMisoPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_3}
const uint32_t | s_SpiMisoModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiSclkPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_0}
const uint32_t | s_SpiSclkModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiIrqSensorPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_12}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) sensor IRQ definitions. More...

## Detailed Description

This file provides all the low level API to manage SDK Version identification.

Author
  AMS VMA RF application team

Version
  V1.0.0

Date
  September 29, 2015

THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.

THIS SOURCE CODE IS PROTECTED BY A LICENSE. FOR MORE INFORMATION PLEASE CAREFULLY READ THE LICENSE AGREEMENT FILE LOCATED IN THE ROOT DIRECTORY OF THIS FIRMWARE PACKAGE.

##
© COPYRIGHT 2015 STMicroelectronics

Definition in file SDK_EVAL_Config.c.