| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Variables
SDK EVAL I2C Private Variable
SDK EVAL BlueNRG1 » SDK EVAL I2C

## Variables

uint8_t | i2c_buffer_tx [I2C_BUFF_SIZE]
| I2C buffers used for DMA application. More...
uint8_t | i2c_buffer_rx [I2C_BUFF_SIZE]
volatile FlagStatus | i2c_eot = SET
| I2C flag set at end of transaction. More...

## Detailed Description

## Variable Documentation

uint8_t i2c_buffer_rx[I2C_BUFF_SIZE]

Definition at line 80 of file SDK_EVAL_I2C.c.

uint8_t i2c_buffer_tx[I2C_BUFF_SIZE]

I2C buffers used for DMA application.

Definition at line 79 of file SDK_EVAL_I2C.c.

volatile FlagStatus i2c_eot = SET

I2C flag set at end of transaction.

Definition at line 85 of file SDK_EVAL_I2C.c.