| BlueNRG-1 ACI APIs and events callbacks

- Main Page
- Modules
- Classes
- Files

Offsets and lengths for configuration values.

Offsets and lengths for configuration values. See aci_hal_write_config_data(). More...

## Configuration values.

See aci_hal_write_config_data().
#define | CONFIG_DATA_PUBADDR_OFFSET (0x00)
#define | CONFIG_DATA_DIV_OFFSET (0x06)
#define | CONFIG_DATA_ER_OFFSET (0x08)
#define | CONFIG_DATA_IR_OFFSET (0x18)
#define | CONFIG_DATA_LL_WITHOUT_HOST (0x2C)
#define | CONFIG_DATA_ROLE (0x2D)

## Length for configuration values.

See aci_hal_write_config_data().
#define | CONFIG_DATA_PUBADDR_LEN (6)
#define | CONFIG_DATA_DIV_LEN (2)
#define | CONFIG_DATA_ER_LEN (16)
#define | CONFIG_DATA_IR_LEN (16)
#define | CONFIG_DATA_LL_WITHOUT_HOST_LEN (1)
#define | CONFIG_DATA_ROLE_LEN (1)

## Detailed Description

Offsets and lengths for configuration values. See aci_hal_write_config_data().

## Macro Definition Documentation

#define CONFIG_DATA_DIV_LEN (2)

Definition at line 63 of file bluenrg1_hal.h.

#define CONFIG_DATA_DIV_OFFSET (0x06)

DIV used to derive CSRK

Definition at line 37 of file bluenrg1_hal.h.

#define CONFIG_DATA_ER_LEN (16)

Definition at line 64 of file bluenrg1_hal.h.

#define CONFIG_DATA_ER_OFFSET (0x08)

Encryption root key used to derive LTK and CSRK

Definition at line 38 of file bluenrg1_hal.h.

#define CONFIG_DATA_IR_LEN (16)

Definition at line 65 of file bluenrg1_hal.h.

#define CONFIG_DATA_IR_OFFSET (0x18)

Identity root key used to derive LTK and CSRK

Definition at line 39 of file bluenrg1_hal.h.

#define CONFIG_DATA_LL_WITHOUT_HOST (0x2C)

Switch on/off Link Layer only mode. Set to 1 to disable Host. It can be written only if aci_hal_write_config_data() is the first command after reset.

Definition at line 40 of file bluenrg1_hal.h.

#define CONFIG_DATA_LL_WITHOUT_HOST_LEN (1)

Definition at line 66 of file bluenrg1_hal.h.

#define CONFIG_DATA_PUBADDR_LEN (6)

Definition at line 62 of file bluenrg1_hal.h.

#define CONFIG_DATA_PUBADDR_OFFSET (0x00)

Bluetooth public address

Definition at line 36 of file bluenrg1_hal.h.

#define CONFIG_DATA_ROLE (0x2D)

Select the BlueNRG roles and mode configurations.

- Mode 1: slave or master, 1 connection, RAM1 only (small GATT DB)
- Mode 2: slave or master, 1 connection, RAM1 and RAM2 (large GATT DB)
- Mode 3: master only, 8 connections, RAM1 and RAM2.

Definition at line 52 of file bluenrg1_hal.h.

#define CONFIG_DATA_ROLE_LEN (1)

Definition at line 67 of file bluenrg1_hal.h.