| BlueNRG-1 Peripherals drivers Examples

- Main Page
- Modules
- Classes
- Files

Macros | Functions | Variables
MTFX Mode 2 Example
BlueNRG1 Standard Peripheral Examples » MTFX Examples

## Macros

#define | IO_CAPTURE_PIN_MFT1_TIMERA 2 /* IO2 */
#define | IO_CAPTURE_PIN_MFT1_TIMERB 3 /* IO3 */

## Functions

void | MFT_Configuration ()
| MFT_Configuration. More...
int | main (void)
| Main program code. More...

## Variables

FlagStatus | fA_found = RESET
FlagStatus | fB_found = RESET

## Detailed Description

## Macro Definition Documentation

#define IO_CAPTURE_PIN_MFT1_TIMERA 2 /* IO2 */

Definition at line 181 of file MFT_Mode_2_main.c.

#define IO_CAPTURE_PIN_MFT1_TIMERB 3 /* IO3 */

Definition at line 182 of file MFT_Mode_2_main.c.

## Function Documentation

int main | ( | void |  | ) |

Main program code.

Parameters

  None |

Return values

  None |

Definition at line 201 of file MFT_Mode_2_main.c.

void MFT_Configuration | ( | void |  | ) |

MFT_Configuration.

Parameters

  None |

Return values

  None |

Definition at line 264 of file MFT_Mode_2_main.c.

## Variable Documentation

FlagStatus fA_found = RESET

Definition at line 186 of file MFT_Mode_2_main.c.

FlagStatus fB_found = RESET

Definition at line 187 of file MFT_Mode_2_main.c.