| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Priority Level Definitions
BLUENRG1 Peripheral Driver » DMA Peripheral » Exported Constants

## Macros

#define | DMA_Priority_VeryHigh ((uint32_t)0x00003000)
#define | DMA_Priority_High ((uint32_t)0x00002000)
#define | DMA_Priority_Medium ((uint32_t)0x00001000)
#define | DMA_Priority_Low ((uint32_t)0x00000000)
#define | IS_DMA_PRIORITY(PRIORITY)

## Detailed Description

## Macro Definition Documentation

#define DMA_Priority_High ((uint32_t)0x00002000)

Definition at line 175 of file BlueNRG1_dma.h.

#define DMA_Priority_Low ((uint32_t)0x00000000)

Definition at line 177 of file BlueNRG1_dma.h.

#define DMA_Priority_Medium ((uint32_t)0x00001000)

Definition at line 176 of file BlueNRG1_dma.h.

#define DMA_Priority_VeryHigh ((uint32_t)0x00003000)

Definition at line 174 of file BlueNRG1_dma.h.

#define IS_DMA_PRIORITY | ( |  | PRIORITY | ) |

Value:
(((PRIORITY) == DMA_Priority_VeryHigh) || \
((PRIORITY) == DMA_Priority_High) || \
((PRIORITY) == DMA_Priority_Medium) || \
((PRIORITY) == DMA_Priority_Low))
DMA_Priority_Low
#define DMA_Priority_Low
Definition: BlueNRG1_dma.h:177
DMA_Priority_VeryHigh
#define DMA_Priority_VeryHigh
Definition: BlueNRG1_dma.h:174
DMA_Priority_High
#define DMA_Priority_High
Definition: BlueNRG1_dma.h:175
DMA_Priority_Medium
#define DMA_Priority_Medium
Definition: BlueNRG1_dma.h:176

Definition at line 178 of file BlueNRG1_dma.h.