| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
UART_InitType Struct Reference
BLUENRG1 Peripheral Driver » UART Peripheral » Exported Types

Structure definition of UART initialization. More...

`#include <BlueNRG1_uart.h>`

## Public Attributes

uint32_t | UART_BaudRate
uint8_t | UART_WordLengthTransmit
uint8_t | UART_WordLengthReceive
uint8_t | UART_StopBits
uint8_t | UART_Parity
uint8_t | UART_Mode
uint8_t | UART_HardwareFlowControl
FunctionalState | UART_FifoEnable

## Detailed Description

Structure definition of UART initialization.

Definition at line 49 of file BlueNRG1_uart.h.

## Member Data Documentation

uint32_t UART_InitType::UART_BaudRate

This member configures the UART communication baud rate.

Definition at line 51 of file BlueNRG1_uart.h.

FunctionalState UART_InitType::UART_FifoEnable

Specifies whether the FIFO is enabled or disabled. This parameter can be a value of UART_Fifo_Enable

Definition at line 72 of file BlueNRG1_uart.h.

uint8_t UART_InitType::UART_HardwareFlowControl

Specifies whether the hardware flow control mode is enabled or disabled. This parameter can be a value of UART_Hardware_Flow_Control

Definition at line 68 of file BlueNRG1_uart.h.

uint8_t UART_InitType::UART_Mode

Specifies whether the Receive or Transmit mode is enabled or disabled. This parameter can be a value of UART_Mode

Definition at line 65 of file BlueNRG1_uart.h.

uint8_t UART_InitType::UART_Parity

Specifies the parity mode. This parameter can be a value of UART_Parity

Definition at line 62 of file BlueNRG1_uart.h.

uint8_t UART_InitType::UART_StopBits

Specifies the number of stop bits transmitted. This parameter can be a value of UART_Stop_Bits

Definition at line 59 of file BlueNRG1_uart.h.

uint8_t UART_InitType::UART_WordLengthReceive

Specifies the number of data bits received in a frame. This parameter can be a value of UART_Word_Length

Definition at line 56 of file BlueNRG1_uart.h.

uint8_t UART_InitType::UART_WordLengthTransmit

Specifies the number of data bits transmitted in a frame. This parameter can be a value of UART_Word_Length

Definition at line 53 of file BlueNRG1_uart.h.

The documentation for this struct was generated from the following file:

- BlueNRG1_uart.h