| BlueNRG-1 ACI APIs and events callbacks

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
hardware_config_table_t Struct Reference

`#include <bluenrg1_stack.h>`

## Public Attributes

uint32_t * | hot_ana_config_table
uint32_t | max_conn_event_length
uint16_t | slave_sca
uint8_t | master_sca
uint8_t | ls_source
uint16_t | hs_startup_time

## Detailed Description

This structure contains low level hardware configuration data for the device

Definition at line 66 of file bluenrg1_stack.h.

## Member Data Documentation

uint32_t* hardware_config_table_t::hot_ana_config_table

Set to NULL

Definition at line 67 of file bluenrg1_stack.h.

uint16_t hardware_config_table_t::hs_startup_time

Start up time of the high speed (16 or 32 MHz) crystal oscillator in units of 625/256 us (~2.44 us)

Definition at line 72 of file bluenrg1_stack.h.

uint8_t hardware_config_table_t::ls_source

Source for the 32 kHz slow speed clock: 1: internal RO; 0: external crystal

Definition at line 71 of file bluenrg1_stack.h.

uint8_t hardware_config_table_t::master_sca

Sleep clock accuracy in Master mode (0 to 7 corresponding to 500, 250, 150, 100, 75, 50, 30, 20 ppm)

Definition at line 70 of file bluenrg1_stack.h.

uint32_t hardware_config_table_t::max_conn_event_length

Maximum duration of the connection event when the device is in Slave mode in units of 625/256 us (~2.44 us)

Definition at line 68 of file bluenrg1_stack.h.

uint16_t hardware_config_table_t::slave_sca

Sleep clock accuracy in Slave mode (ppm value)

Definition at line 69 of file bluenrg1_stack.h.

The documentation for this struct was generated from the following file:

- bluenrg1_stack.h