| BlueNRG-1 Master/Central Library

- Main Page
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
dataPermitExchangeS Struct Reference

Data received from the peer peripheral device when a write or a read request is received and the application has set the permit request event in the characteristic. More...

`#include <master_basic_profile.h>`

## Public Attributes

uint16_t | attr_handle
uint8_t | data_length
uint8_t * | data
uint8_t | offset

## Detailed Description

Data received from the peer peripheral device when a write or a read request is received and the application has set the permit request event in the characteristic.

Definition at line 480 of file master_basic_profile.h.

## Member Data Documentation

uint16_t dataPermitExchangeS::attr_handle

The handle of the attribute for which the read request has been made by the client

Definition at line 482 of file master_basic_profile.h.

uint8_t* dataPermitExchangeS::data

The data that the client has requested to write. It is not used in case of read permit procedure

Definition at line 486 of file master_basic_profile.h.

uint8_t dataPermitExchangeS::data_length

Length of data field for write permit procedure. In case of read permit procedure is always 1

Definition at line 484 of file master_basic_profile.h.

uint8_t dataPermitExchangeS::offset

Contains the offset from which the read permit procedure has been requested. It is not used in case of write permit procedure

Definition at line 488 of file master_basic_profile.h.

The documentation for this struct was generated from the following file:

- master_basic_profile.h