| STM32L - BlueNRG-1 BLE stack APIs, Events and Constants

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

bluenrg1_l2cap_aci.h
Go to the documentation of this file.
1 #ifndef __BLUENRG1_L2CAP_ACI_H__
2 #define __BLUENRG1_L2CAP_ACI_H__
3
4
25 #include "bluenrg1_types.h"
49 tBleStatus aci_l2cap_connection_parameter_update_req(uint16_t Connection_Handle,
50 uint16_t Conn_Interval_Min,
51 uint16_t Conn_Interval_Max,
52 uint16_t Slave_latency,
53 uint16_t Timeout_Multiplier);
88 tBleStatus aci_l2cap_connection_parameter_update_resp(uint16_t Connection_Handle,
89 uint16_t Conn_Interval_Min,
90 uint16_t Conn_Interval_Max,
91 uint16_t Slave_latency,
92 uint16_t Timeout_Multiplier,
93 uint16_t Minimum_CE_Length,
94 uint16_t Maximum_CE_Length,
95 uint8_t Identifier,
96 uint8_t Accept);
100 #endif /* __BLUENRG1_L2CAP_ACI_H__*/
aci_l2cap_connection_parameter_update_resp
tBleStatus aci_l2cap_connection_parameter_update_resp(uint16_t Connection_Handle, uint16_t Conn_Interval_Min, uint16_t Conn_Interval_Max, uint16_t Slave_latency, uint16_t Timeout_Multiplier, uint16_t Minimum_CE_Length, uint16_t Maximum_CE_Length, uint8_t Identifier, uint8_t Accept)
Accept or reject a connection update. This command should be sent in response to a aci_l2cap_connecti...
aci_l2cap_connection_parameter_update_req
tBleStatus aci_l2cap_connection_parameter_update_req(uint16_t Connection_Handle, uint16_t Conn_Interval_Min, uint16_t Conn_Interval_Max, uint16_t Slave_latency, uint16_t Timeout_Multiplier)
Send an L2CAP connection parameter update request from the slave to the master. An aci_l2cap_connecti...