| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Interrupts Definitions
BLUENRG1 Peripheral Driver » RTC Peripheral » Exported Constants

## Macros

#define | RTC_IT_CLOCKWATCH ((uint8_t)1)
#define | RTC_IT_TIMER ((uint8_t)2)
#define | IS_RTC_IT(IT)

## Detailed Description

## Macro Definition Documentation

#define IS_RTC_IT | ( |  | IT | ) |

Value:
(((IT) == RTC_IT_CLOCKWATCH) || \
((IT) == RTC_IT_TIMER))
RTC_IT_CLOCKWATCH
#define RTC_IT_CLOCKWATCH
Definition: BlueNRG1_rtc.h:162
RTC_IT_TIMER
#define RTC_IT_TIMER
Definition: BlueNRG1_rtc.h:163

This macro checks if IT is a valid combination of interrupt

Definition at line 167 of file BlueNRG1_rtc.h.

#define RTC_IT_CLOCKWATCH ((uint8_t)1)

RTC clock watch interrupt

Definition at line 162 of file BlueNRG1_rtc.h.

#define RTC_IT_TIMER ((uint8_t)2)

RTC timer interrupt

Definition at line 163 of file BlueNRG1_rtc.h.