| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Interrupts Channel Definitions
BLUENRG1 Peripheral Driver » DMA Peripheral » Exported Constants

## Macros

#define | DMA_FLAG_GL0 ((uint32_t)0x00000001)
#define | DMA_FLAG_TC0 ((uint32_t)0x00000002)
#define | DMA_FLAG_HT0 ((uint32_t)0x00000004)
#define | DMA_FLAG_TE0 ((uint32_t)0x00000008)
#define | DMA_FLAG_GL1 ((uint32_t)0x00000010)
#define | DMA_FLAG_TC1 ((uint32_t)0x00000020)
#define | DMA_FLAG_HT1 ((uint32_t)0x00000040)
#define | DMA_FLAG_TE1 ((uint32_t)0x00000080)
#define | DMA_FLAG_GL2 ((uint32_t)0x00000100)
#define | DMA_FLAG_TC2 ((uint32_t)0x00000200)
#define | DMA_FLAG_HT2 ((uint32_t)0x00000400)
#define | DMA_FLAG_TE2 ((uint32_t)0x00000800)
#define | DMA_FLAG_GL3 ((uint32_t)0x00001000)
#define | DMA_FLAG_TC3 ((uint32_t)0x00002000)
#define | DMA_FLAG_HT3 ((uint32_t)0x00004000)
#define | DMA_FLAG_TE3 ((uint32_t)0x00008000)
#define | DMA_FLAG_GL4 ((uint32_t)0x00010000)
#define | DMA_FLAG_TC4 ((uint32_t)0x00020000)
#define | DMA_FLAG_HT4 ((uint32_t)0x00040000)
#define | DMA_FLAG_TE4 ((uint32_t)0x00080000)
#define | DMA_FLAG_GL5 ((uint32_t)0x00100000)
#define | DMA_FLAG_TC5 ((uint32_t)0x00200000)
#define | DMA_FLAG_HT5 ((uint32_t)0x00400000)
#define | DMA_FLAG_TE5 ((uint32_t)0x00800000)
#define | DMA_FLAG_GL6 ((uint32_t)0x01000000)
#define | DMA_FLAG_TC6 ((uint32_t)0x02000000)
#define | DMA_FLAG_HT6 ((uint32_t)0x04000000)
#define | DMA_FLAG_TE6 ((uint32_t)0x08000000)
#define | DMA_FLAG_GL7 ((uint32_t)0x10000000)
#define | DMA_FLAG_TC7 ((uint32_t)0x20000000)
#define | DMA_FLAG_HT7 ((uint32_t)0x40000000)
#define | DMA_FLAG_TE7 ((uint32_t)0x80000000)
#define | IS_DMA_CH_FLAG(FLAG) ((FLAG) != 0x00)
#define | DMA_ADC_CHANNEL0 ((uint8_t)0x01)
#define | DMA_ADC_CHANNEL1 ((uint8_t)0x02)
#define | DMA_ADC_CHANNEL2 ((uint8_t)0x04)
#define | DMA_ADC_CHANNEL3 ((uint8_t)0x08)
#define | DMA_ADC_CHANNEL4 ((uint8_t)0x10)
#define | DMA_ADC_CHANNEL5 ((uint8_t)0x20)
#define | DMA_ADC_CHANNEL6 ((uint8_t)0x40)
#define | DMA_ADC_CHANNEL7 ((uint8_t)0x80)
#define | IS_DMA_ADC_CH(SEL)

## Detailed Description

## Macro Definition Documentation

#define DMA_ADC_CHANNEL0 ((uint8_t)0x01)

Definition at line 264 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL1 ((uint8_t)0x02)

Definition at line 265 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL2 ((uint8_t)0x04)

Definition at line 266 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL3 ((uint8_t)0x08)

Definition at line 267 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL4 ((uint8_t)0x10)

Definition at line 268 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL5 ((uint8_t)0x20)

Definition at line 269 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL6 ((uint8_t)0x40)

Definition at line 270 of file BlueNRG1_dma.h.

#define DMA_ADC_CHANNEL7 ((uint8_t)0x80)

Definition at line 271 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL0 ((uint32_t)0x00000001)

Definition at line 216 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL1 ((uint32_t)0x00000010)

Definition at line 220 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL2 ((uint32_t)0x00000100)

Definition at line 224 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL3 ((uint32_t)0x00001000)

Definition at line 228 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL4 ((uint32_t)0x00010000)

Definition at line 232 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL5 ((uint32_t)0x00100000)

Definition at line 236 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL6 ((uint32_t)0x01000000)

Definition at line 240 of file BlueNRG1_dma.h.

#define DMA_FLAG_GL7 ((uint32_t)0x10000000)

Definition at line 244 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT0 ((uint32_t)0x00000004)

Definition at line 218 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT1 ((uint32_t)0x00000040)

Definition at line 222 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT2 ((uint32_t)0x00000400)

Definition at line 226 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT3 ((uint32_t)0x00004000)

Definition at line 230 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT4 ((uint32_t)0x00040000)

Definition at line 234 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT5 ((uint32_t)0x00400000)

Definition at line 238 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT6 ((uint32_t)0x04000000)

Definition at line 242 of file BlueNRG1_dma.h.

#define DMA_FLAG_HT7 ((uint32_t)0x40000000)

Definition at line 246 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC0 ((uint32_t)0x00000002)

Definition at line 217 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC1 ((uint32_t)0x00000020)

Definition at line 221 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC2 ((uint32_t)0x00000200)

Definition at line 225 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC3 ((uint32_t)0x00002000)

Definition at line 229 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC4 ((uint32_t)0x00020000)

Definition at line 233 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC5 ((uint32_t)0x00200000)

Definition at line 237 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC6 ((uint32_t)0x02000000)

Definition at line 241 of file BlueNRG1_dma.h.

#define DMA_FLAG_TC7 ((uint32_t)0x20000000)

Definition at line 245 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE0 ((uint32_t)0x00000008)

Definition at line 219 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE1 ((uint32_t)0x00000080)

Definition at line 223 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE2 ((uint32_t)0x00000800)

Definition at line 227 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE3 ((uint32_t)0x00008000)

Definition at line 231 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE4 ((uint32_t)0x00080000)

Definition at line 235 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE5 ((uint32_t)0x00800000)

Definition at line 239 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE6 ((uint32_t)0x08000000)

Definition at line 243 of file BlueNRG1_dma.h.

#define DMA_FLAG_TE7 ((uint32_t)0x80000000)

Definition at line 247 of file BlueNRG1_dma.h.

#define IS_DMA_ADC_CH | ( |  | SEL | ) |

Value:
(((SEL) == DMA_ADC_CHANNEL0) || \
((SEL) == DMA_ADC_CHANNEL1) || \
((SEL) == DMA_ADC_CHANNEL2) || \
((SEL) == DMA_ADC_CHANNEL3) || \
((SEL) == DMA_ADC_CHANNEL4) || \
((SEL) == DMA_ADC_CHANNEL5) || \
((SEL) == DMA_ADC_CHANNEL6) || \
((SEL) == DMA_ADC_CHANNEL7))
DMA_ADC_CHANNEL2
#define DMA_ADC_CHANNEL2
Definition: BlueNRG1_dma.h:266
DMA_ADC_CHANNEL0
#define DMA_ADC_CHANNEL0
Definition: BlueNRG1_dma.h:264
DMA_ADC_CHANNEL5
#define DMA_ADC_CHANNEL5
Definition: BlueNRG1_dma.h:269
DMA_ADC_CHANNEL6
#define DMA_ADC_CHANNEL6
Definition: BlueNRG1_dma.h:270
DMA_ADC_CHANNEL4
#define DMA_ADC_CHANNEL4
Definition: BlueNRG1_dma.h:268
DMA_ADC_CHANNEL7
#define DMA_ADC_CHANNEL7
Definition: BlueNRG1_dma.h:271
DMA_ADC_CHANNEL3
#define DMA_ADC_CHANNEL3
Definition: BlueNRG1_dma.h:267
DMA_ADC_CHANNEL1
#define DMA_ADC_CHANNEL1
Definition: BlueNRG1_dma.h:265

Definition at line 274 of file BlueNRG1_dma.h.

#define IS_DMA_CH_FLAG | ( |  | FLAG | ) | ((FLAG) != 0x00)

Definition at line 250 of file BlueNRG1_dma.h.