| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

- All
- Functions
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- f
- g
- h
- i
- l
- m
- n
- r
- s
- u
- w
- x

Here is a list of all file members with links to the files they belong to:

### - i -

- I2C_AddressType_10Bit : BlueNRG1_i2c.h
- I2C_AddressType_7Bit : BlueNRG1_i2c.h
- I2C_AddressType_GeneralCall : BlueNRG1_i2c.h
- I2C_BeginTransaction() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_ClearITPendingBit() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_CLOCK : BlueNRG1_i2c.c
- I2C_Cmd() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_CR_SM_FAST : BlueNRG1_i2c.c
- I2C_CR_SM_STD : BlueNRG1_i2c.c
- I2C_DeInit() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_DMACmd() : BlueNRG1_i2c.c , BlueNRG1_i2c.h
- I2C_DMAReq_Rx : BlueNRG1_i2c.h
- I2C_DMAReq_Tx : BlueNRG1_i2c.h
- I2C_DMATxBurstMode() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_DMATxBurstSize() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_FillTxFIFO() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_Filtering_1Ck_Spike : BlueNRG1_i2c.h
- I2C_Filtering_2Ck_Spikes : BlueNRG1_i2c.h
- I2C_Filtering_4Ck_Spikes : BlueNRG1_i2c.h
- I2C_Filtering_Off : BlueNRG1_i2c.h
- I2C_FlushRx() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_FlushTx() : BlueNRG1_i2c.c , BlueNRG1_i2c.h
- I2C_GeneralCallCmd() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_GenerateStopCondition() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_GetITPendingBit() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_GetITStatus() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_GetStatus() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_Init() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_IT_BERR : BlueNRG1_i2c.h
- I2C_IT_LBR : BlueNRG1_i2c.h
- I2C_IT_MAL : BlueNRG1_i2c.h
- I2C_IT_MSK : BlueNRG1_i2c.h
- I2C_IT_MTD : BlueNRG1_i2c.h
- I2C_IT_MTDWS : BlueNRG1_i2c.h
- I2C_IT_RFSE : BlueNRG1_i2c.h
- I2C_IT_RFSR : BlueNRG1_i2c.h
- I2C_IT_RXFE : BlueNRG1_i2c.h
- I2C_IT_RXFF : BlueNRG1_i2c.h
- I2C_IT_RXFNF : BlueNRG1_i2c.h
- I2C_IT_SAL : BlueNRG1_i2c.h
- I2C_IT_STD : BlueNRG1_i2c.h
- I2C_IT_TIMEOUT : BlueNRG1_i2c.h
- I2C_IT_TXFE : BlueNRG1_i2c.h
- I2C_IT_TXFF : BlueNRG1_i2c.h
- I2C_IT_TXFNE : BlueNRG1_i2c.h
- I2C_IT_TXFOVR : BlueNRG1_i2c.h
- I2C_IT_WTSR : BlueNRG1_i2c.h
- I2C_ITConfig() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_NOP : BlueNRG1_i2c.h
- I2C_OP_ABORTED : BlueNRG1_i2c.h
- I2C_OP_OK : BlueNRG1_i2c.h
- I2C_OP_ONGOING : BlueNRG1_i2c.h
- I2C_OperatingMode_Master : BlueNRG1_i2c.h
- I2C_OperatingMode_MasterSlave : BlueNRG1_i2c.h
- I2C_OperatingMode_Slave : BlueNRG1_i2c.h
- I2C_Operation_Read : BlueNRG1_i2c.h
- I2C_Operation_Write : BlueNRG1_i2c.h
- I2C_OpStatus : BlueNRG1_i2c.h
- I2C_ReceiveData() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_SetHoldTime() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_SetHoldTimeStartCondition() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_SetRxThreshold() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_SetTxThreshold() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_SLAVE_ADDR_EXT10_SMK : BlueNRG1_i2c.c
- I2C_StartByte_Disable : BlueNRG1_i2c.h
- I2C_StartByte_Enable : BlueNRG1_i2c.h
- I2C_StopCondition_Disable : BlueNRG1_i2c.h
- I2C_StopCondition_Enable : BlueNRG1_i2c.h
- I2C_StructInit() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_WaitFlushRx() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- I2C_WaitFlushTx() : BlueNRG1_i2c.h , BlueNRG1_i2c.c
- IS_ADC_ATTENUATION : BlueNRG1_adc.h
- IS_ADC_CONVERSIONMODE : BlueNRG1_adc.h
- IS_ADC_DECIMATIONRATE : BlueNRG1_adc.h
- IS_ADC_GET_FLAG : BlueNRG1_adc.h
- IS_ADC_INPUT : BlueNRG1_adc.h
- IS_ADC_MIC_FREQ_SEL : BlueNRG1_adc.h
- IS_ADC_REFERENCEVOLTAGE : BlueNRG1_adc.h
- IS_CLOCK_PERIPH : BlueNRG1_sysCtrl.h
- IS_DMA_ADC_CH : BlueNRG1_dma.h
- IS_DMA_ALL_PERIPH : BlueNRG1_dma.c
- IS_DMA_BUFFER_SIZE : BlueNRG1_dma.h
- IS_DMA_CH_FLAG : BlueNRG1_dma.h
- IS_DMA_CONFIG_FLAG : BlueNRG1_dma.h
- IS_DMA_DIR : BlueNRG1_dma.h
- IS_DMA_M2M_STATE : BlueNRG1_dma.h
- IS_DMA_MEMORY_DATA_SIZE : BlueNRG1_dma.h
- IS_DMA_MEMORY_INC_STATE : BlueNRG1_dma.h
- IS_DMA_MODE : BlueNRG1_dma.h
- IS_DMA_PERIPHERAL_DATA_SIZE : BlueNRG1_dma.h
- IS_DMA_PERIPHERAL_INC_STATE : BlueNRG1_dma.h
- IS_DMA_PRIORITY : BlueNRG1_dma.h
- IS_FIFO_LEV : BlueNRG1_uart.h
- IS_FLASH_ADDRESS : BlueNRG1_flash.h
- IS_FLASH_CMD : BlueNRG1_flash.h
- IS_FLASH_FLAG : BlueNRG1_flash.h
- IS_GPIO_BIT_ACTION : BlueNRG1_gpio.h
- IS_GPIO_EVENT : BlueNRG1_gpio.h
- IS_GPIO_IRQSENSE : BlueNRG1_gpio.h
- IS_GPIO_MODE : BlueNRG1_gpio.h
- IS_GPIO_PIN : BlueNRG1_gpio.h
- IS_GPIO_PINS : BlueNRG1_gpio.h
- IS_HOUR : BlueNRG1_rtc.h
- IS_I2C_ADDRESSTYPE : BlueNRG1_i2c.h
- IS_I2C_ALL_PERIPH : BlueNRG1_i2c.h
- IS_I2C_BURSTSIZE : BlueNRG1_i2c.h
- IS_I2C_CLOCK_SPEED_I2C : BlueNRG1_i2c.h
- IS_I2C_DMAREQ : BlueNRG1_i2c.h
- IS_I2C_FILTERING : BlueNRG1_i2c.h
- IS_I2C_HOLDTIME : BlueNRG1_i2c.h
- IS_I2C_IT : BlueNRG1_i2c.h
- IS_I2C_LENGTH : BlueNRG1_i2c.h
- IS_I2C_OPERATING_MODE : BlueNRG1_i2c.h
- IS_I2C_OPERATION : BlueNRG1_i2c.h
- IS_I2C_OWN_ADDRESS : BlueNRG1_i2c.h
- IS_I2C_OWN_ADDRESS1 : BlueNRG1_i2c.h
- IS_I2C_RX_THRESHOLD : BlueNRG1_i2c.h
- IS_I2C_STARTBYTE : BlueNRG1_i2c.h
- IS_I2C_STOPCONDITION : BlueNRG1_i2c.h
- IS_I2C_TX_THRESHOLD : BlueNRG1_i2c.h
- IS_MATCH_MONTH : BlueNRG1_rtc.h
- IS_MATCH_MONTHDAY : BlueNRG1_rtc.h
- IS_MATCH_WEEKDAY : BlueNRG1_rtc.h
- IS_MATCH_YEAR : BlueNRG1_rtc.h
- IS_MFT : BlueNRG1_mft.h
- IS_MFT_CLOCK_SEL : BlueNRG1_mft.h
- IS_MFT_INPUT_IO : BlueNRG1_mft.h
- IS_MFT_INTERRUPT : BlueNRG1_mft.h
- IS_MFT_MODE : BlueNRG1_mft.h
- IS_MFT_PULSETRAIN_TRIGGER : BlueNRG1_mft.h
- IS_MFT_PWMX_PIN : BlueNRG1_mft.h
- IS_MFT_TIMER : BlueNRG1_mft.h
- IS_MFT_Tn_EDGE : BlueNRG1_mft.h
- IS_MFT_TnX : BlueNRG1_mft.h
- IS_MINUTE : BlueNRG1_rtc.h
- IS_MONTH : BlueNRG1_rtc.h
- IS_MONTHDAY : BlueNRG1_rtc.h
- IS_NVIC_PREEMPTION_PRIORITY : misc.h
- IS_PAGE_NUMBER : BlueNRG1_flash.h
- IS_PATTERN : BlueNRG1_rtc.h
- IS_ROW_NUMBER : BlueNRG1_flash.h
- IS_RTC_IT : BlueNRG1_rtc.h
- IS_RTC_TIMER_MODE : BlueNRG1_rtc.h
- IS_SECOND : BlueNRG1_rtc.h
- IS_SPI_BAUDRATE : BlueNRG1_spi.h
- IS_SPI_CLEAR_IT : BlueNRG1_spi.h
- IS_SPI_COM_MODE : BlueNRG1_spi.h
- IS_SPI_CONFIG_IT : BlueNRG1_spi.h
- IS_SPI_CPHA : BlueNRG1_spi.h
- IS_SPI_CPOL : BlueNRG1_spi.h
- IS_SPI_DATASIZE : BlueNRG1_spi.h
- IS_SPI_DMAREQ : BlueNRG1_spi.h
- IS_SPI_ENDIAN : BlueNRG1_spi.h
- IS_SPI_FIFO_LEV : BlueNRG1_spi.h
- IS_SPI_GET_FLAG : BlueNRG1_spi.h
- IS_SPI_GET_IT : BlueNRG1_spi.h
- IS_SPI_MODE : BlueNRG1_spi.h
- IS_SW_FLOW_CTRL : BlueNRG1_uart.h
- IS_UART_BAUDRATE : BlueNRG1_uart.h
- IS_UART_CLEAR_FLAG : BlueNRG1_uart.h
- IS_UART_CONFIG_IT : BlueNRG1_uart.h
- IS_UART_DATA : BlueNRG1_uart.h
- IS_UART_DMAREQ : BlueNRG1_uart.h
- IS_UART_FLAG : BlueNRG1_uart.h
- IS_UART_HW_FLOW_CONTROL : BlueNRG1_uart.h
- IS_UART_MODE : BlueNRG1_uart.h
- IS_UART_PARITY : BlueNRG1_uart.h
- IS_UART_STOPBITS : BlueNRG1_uart.h
- IS_UART_TIMEOUT : BlueNRG1_uart.h
- IS_UART_WORD_LENGTH : BlueNRG1_uart.h
- IS_WAIT_VALUE : BlueNRG1_spi.h
- IS_WAKEUP_ON_IO : BlueNRG1_sysCtrl.h
- IS_WAKEUP_ON_STATE : BlueNRG1_sysCtrl.h
- IS_WEEKDAY : BlueNRG1_rtc.h
- IS_WORD_NUMBER : BlueNRG1_flash.h
- IS_XO_FREQ : BlueNRG1_sysCtrl.h
- IS_YEAR : BlueNRG1_rtc.h