| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

- All
- Functions
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- f
- g
- h
- i
- l
- m
- n
- r
- s
- u
- w
- x

Here is a list of all file members with links to the files they belong to:

### - a -

- ADC_Attenuation_0dB : BlueNRG1_adc.h
- ADC_Attenuation_6dB02 : BlueNRG1_adc.h
- ADC_Attenuation_9dB54 : BlueNRG1_adc.h
- ADC_AutoOffsetUpdate() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_Calibration() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_Cmd() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ConversionMode() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ConversionMode_Continuous : BlueNRG1_adc.h
- ADC_ConversionMode_Single : BlueNRG1_adc.h
- ADC_ConvertBatterySensor() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ConvertDifferentialVoltage() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ConvertSingleEndedVoltage() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ConvertTemperatureSensor() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_DecimationRate_100 : BlueNRG1_adc.h
- ADC_DecimationRate_200 : BlueNRG1_adc.h
- ADC_DecimationRate_32 : BlueNRG1_adc.h
- ADC_DecimationRate_64 : BlueNRG1_adc.h
- ADC_DeInit() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_DmaCmd() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_FLAG_BUSY : BlueNRG1_adc.h
- ADC_FLAG_CAL : BlueNRG1_adc.h
- ADC_FLAG_EOC : BlueNRG1_adc.h
- ADC_FLAG_WDG : BlueNRG1_adc.h
- ADC_GetConvertedData() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_GetFlagStatus() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_GetITStatus() : BlueNRG1_adc.c , BlueNRG1_adc.h
- ADC_GetRawData : BlueNRG1_adc.h
- ADC_Init() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_Input_AdcPin1 : BlueNRG1_adc.h
- ADC_Input_AdcPin12 : BlueNRG1_adc.h
- ADC_Input_AdcPin2 : BlueNRG1_adc.h
- ADC_Input_BattSensor : BlueNRG1_adc.h
- ADC_Input_Internal0V60V6 : BlueNRG1_adc.h
- ADC_Input_Internal1V20V0 : BlueNRG1_adc.h
- ADC_Input_Microphone : BlueNRG1_adc.h
- ADC_Input_None : BlueNRG1_adc.h
- ADC_Input_TempSensor : BlueNRG1_adc.h
- ADC_ITConfig() : BlueNRG1_adc.c , BlueNRG1_adc.h
- ADC_MIC_1600KHZ : BlueNRG1_adc.h
- ADC_MIC_800KHZ : BlueNRG1_adc.h
- ADC_ReferenceVoltage_0V : BlueNRG1_adc.h
- ADC_ReferenceVoltage_0V4 : BlueNRG1_adc.h
- ADC_ReferenceVoltage_0V6 : BlueNRG1_adc.h
- ADC_ReferenceVoltage_1V2 : BlueNRG1_adc.h
- ADC_RoundConvertedData() : BlueNRG1_adc.c , BlueNRG1_adc.h
- ADC_SelectFrequencyMic() : BlueNRG1_adc.c , BlueNRG1_adc.h
- ADC_StructInit() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ThresholdCheck() : BlueNRG1_adc.h , BlueNRG1_adc.c
- ADC_ThresholdConfig() : BlueNRG1_adc.h , BlueNRG1_adc.c
- AIRCR_VECTKEY_MASK : misc.c