| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Functions
Private Functions
BLUENRG1 Peripheral Driver » SPI Peripheral

## Functions

void | SPI_SetBaudrate (uint32_t Baudrate)
| SPI set baud rate function. More...

## Detailed Description

## Function Documentation

void SPI_SetBaudrate | ( | uint32_t | Baudrate | ) |

SPI set baud rate function.

Parameters

  Baudrate | the SPI baud rate up to 8MHz for master mode and 1MHz for slave mode.

Return values

  None |

Definition at line 90 of file BlueNRG1_spi.c.