| BlueNRG-1 Peripherals drivers Examples

- Main Page
- Modules
- Classes
- Files

Macros | Functions | Variables
GPIO Input Interrupt Example
BlueNRG1 Standard Peripheral Examples » GPIO Examples

## Macros

#define | SYST_CLOCK 16000000

## Functions

int | main (void)
| Main program code. More...
void | SdkDelayMs (volatile uint32_t lTimeMs)
| Delay function. More...

## Variables

volatile uint32_t | lSystickCounter =0

## Detailed Description

## Macro Definition Documentation

#define SYST_CLOCK 16000000

Definition at line 153 of file GPIO_IOToggle_main.c.

## Function Documentation

int main | ( | void |  | ) |

Main program code.

Parameters

  None |

Return values

  None |

Definition at line 183 of file GPIO_InputInterrupt_main.c.

void SdkDelayMs | ( | volatile uint32_t | lTimeMs | ) |

Delay function.

Parameters

  Delay | in ms

Return values

  None |

Definition at line 202 of file GPIO_IOToggle_main.c.

## Variable Documentation

volatile uint32_t lSystickCounter =0

Definition at line 157 of file GPIO_IOToggle_main.c.