| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- b
- d
- e
- i
- l
- n
- p
- r
- s
- u

Here is a list of all file members with links to the files they belong to:

### - s -

- s_I2CBaseVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cClkPinModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_I2cClkPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataDmaRxTcVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_I2cDataDmaRxVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataDmaTxTcVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataDmaTxVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_I2cDataPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cPeripheralVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs1ModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs1PinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs2ModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs2PinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiIrqSensorPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiMisoModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_SpiMisoPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiMosiModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiMosiPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiSclkModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiSclkPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_UartRxModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_UartRxPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_UartTxModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_UartTxPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_vectnButtonPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_vectnGpioPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- SDK_EVAL_I2C : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_BASE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_CLK_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_CLK_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_DATA_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_DATA_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_DMA_RX : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_DMA_RX_ITTC : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_DMA_TX : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_DMA_TX_ITTC : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_I2C_IRQ_HANDLER : USER_Platform_Configuration.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_IRQ_SENSOR_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_LED1_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_LED2_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_LED3_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_CS_HIGH : SDK_EVAL_SPI.h
- SDK_EVAL_SPI_CS_LOW : SDK_EVAL_SPI.h
- SDK_EVAL_SPI_PERIPH_MISO_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_MISO_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_MOSI_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_MOSI_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_SCLK_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_SCLK_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_SENSOR_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_SPI_PERIPH_SENSOR_PIN : USER_Platform_Configuration_auto.h , USER_Platform_Configuration.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_UART_RX_MODE : USER_Platform_Configuration_STEVAL_IDB007V1.h , USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h
- SDK_EVAL_UART_RX_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_UART_TX_MODE : USER_Platform_Configuration.h , USER_Platform_Configuration_auto.h , USER_Platform_Configuration_STEVAL_IDB007V1.h
- SDK_EVAL_UART_TX_PIN : USER_Platform_Configuration.h , USER_Platform_Configuration_STEVAL_IDB007V1.h , USER_Platform_Configuration_auto.h
- SDK_PLATFORMS_NUMBER : SDK_EVAL_Config.h
- SdkEvalButton : SDK_EVAL_Button.h
- SdkEvalButtonIrq : SDK_EVAL_Button.h
- SdkEvalComIOConfig() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalComIOProcessInputData() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalComIOReceiveData() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalComIOSendData() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalComIOUartIrqHandler() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalComUartInit() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalComUartIrqConfig() : SDK_EVAL_Com.h , SDK_EVAL_Com.c
- SdkEvalGetVersion() : SDK_EVAL_Config.h , SDK_EVAL_Config.c
- SdkEvalI2CDmaInit() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CDmaRead() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CDmaWrite() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CInit() : SDK_EVAL_I2C.c , SDK_EVAL_I2C.h
- SdkEvalI2CIrqInit() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CIrqRead() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CIrqWrite() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CRead() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalI2CWrite() : SDK_EVAL_I2C.h , SDK_EVAL_I2C.c
- SdkEvalIdentification() : SDK_EVAL_Config.h , SDK_EVAL_Config.c
- SdkEvalLed : SDK_EVAL_Led.h
- SdkEvalLedGetState() : SDK_EVAL_Led.h , SDK_EVAL_Led.c
- SdkEvalLedInit() : SDK_EVAL_Led.c , SDK_EVAL_Led.h
- SdkEvalLedOff() : SDK_EVAL_Led.h , SDK_EVAL_Led.c
- SdkEvalLedOn() : SDK_EVAL_Led.c , SDK_EVAL_Led.h
- SdkEvalLedToggle() : SDK_EVAL_Led.h , SDK_EVAL_Led.c
- SdkEvalPushButtonClearITPendingBit() : SDK_EVAL_Button.h , SDK_EVAL_Button.c
- SdkEvalPushButtonGetITPendingBit() : SDK_EVAL_Button.c , SDK_EVAL_Button.h
- SdkEvalPushButtonGetState() : SDK_EVAL_Button.h , SDK_EVAL_Button.c
- SdkEvalPushButtonInit() : SDK_EVAL_Button.c , SDK_EVAL_Button.h
- SdkEvalPushButtonIrq() : SDK_EVAL_Button.h , SDK_EVAL_Button.c
- SdkEvalSpiDmaInit() : SDK_EVAL_SPI.h , SDK_EVAL_SPI.c
- SdkEvalSpiDmaRead() : SDK_EVAL_SPI.c , SDK_EVAL_SPI.h
- SdkEvalSpiDmaWrite() : SDK_EVAL_SPI.c , SDK_EVAL_SPI.h
- SdkEvalSpiInit() : SDK_EVAL_SPI.h , SDK_EVAL_SPI.c
- SdkEvalSpiIrqInit() : SDK_EVAL_SPI.h , SDK_EVAL_SPI.c
- SdkEvalSpiIrqRead() : SDK_EVAL_SPI.c , SDK_EVAL_SPI.h
- SdkEvalSpiIrqWrite() : SDK_EVAL_SPI.c , SDK_EVAL_SPI.h
- SdkEvalSpiRead() : SDK_EVAL_SPI.h , SDK_EVAL_SPI.c
- SdkEvalSpiWrite() : SDK_EVAL_SPI.h , SDK_EVAL_SPI.c
- SEND_READ_REG : SDK_EVAL_SPI.c
- SEND_START : SDK_EVAL_SPI.c
- SEND_WRITE_DATA : SDK_EVAL_SPI.c
- SEND_WRITE_REG : SDK_EVAL_SPI.c
- SPI_BAUDRATE : SDK_EVAL_SPI.h
- SPI_BUFF_SIZE : SDK_EVAL_SPI.h
- spi_buffer_rx : SDK_EVAL_SPI.c
- spi_buffer_tx : SDK_EVAL_SPI.c
- SPI_DR_BASE_ADDR : SDK_EVAL_SPI.h
- spi_eot : SDK_EVAL_SPI.c
- STEVAL_IDB007V1 : SDK_EVAL_Config.h
- STEVAL_IDB007VX : SDK_EVAL_Config.h