| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Hardware Flow Control Definition
BLUENRG1 Peripheral Driver » UART Peripheral » Exported Constants

## Macros

#define | UART_HardwareFlowControl_None ((uint8_t)0x00)
#define | UART_HardwareFlowControl_RTS ((uint8_t)0x01)
#define | UART_HardwareFlowControl_CTS ((uint8_t)0x02)
#define | UART_HardwareFlowControl_RTS_CTS ((uint8_t)0x03)
#define | IS_UART_HW_FLOW_CONTROL(CONTROL) ( (CONTROL) <= 3 )

## Detailed Description

## Macro Definition Documentation

#define IS_UART_HW_FLOW_CONTROL | ( |  | CONTROL | ) | ( (CONTROL) <= 3 )

Definition at line 156 of file BlueNRG1_uart.h.

#define UART_HardwareFlowControl_CTS ((uint8_t)0x02)

Enables the CTS hardware flow control

Definition at line 152 of file BlueNRG1_uart.h.

#define UART_HardwareFlowControl_None ((uint8_t)0x00)

Disable the hardware flow control

Definition at line 150 of file BlueNRG1_uart.h.

#define UART_HardwareFlowControl_RTS ((uint8_t)0x01)

Enables the RTS hardware flow control

Definition at line 151 of file BlueNRG1_uart.h.

#define UART_HardwareFlowControl_RTS_CTS ((uint8_t)0x03)

Enables the RTS and CTS hardware flow control

Definition at line 153 of file BlueNRG1_uart.h.