| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
RTC_InitType Struct Reference
BLUENRG1 Peripheral Driver » RTC Peripheral » Exported Types

Structure definition of RTC initialization. More...

`#include <BlueNRG1_rtc.h>`

## Public Attributes

uint8_t | RTC_operatingMode
uint32_t | RTC_TLR1
uint32_t | RTC_TLR2
uint32_t | RTC_PATTERN_SIZE
uint32_t | RTC_PATTERN1
uint32_t | RTC_PATTERN2
uint32_t | RTC_PATTERN3
uint32_t | RTC_PATTERN4

## Detailed Description

Structure definition of RTC initialization.

Definition at line 49 of file BlueNRG1_rtc.h.

## Member Data Documentation

uint8_t RTC_InitType::RTC_operatingMode

Specifies the operating mode. This parameter can be a value of RTC_Timer_OperatingMode

Definition at line 51 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_PATTERN1

Define the pattern, '0' relaod TLR1 and '1' reload TLR2. First 32 bit pattern

Definition at line 63 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_PATTERN2

Define the pattern, '0' relaod TLR1 and '1' reload TLR2. Second 32 bit pattern

Definition at line 66 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_PATTERN3

Define the pattern, '0' relaod TLR1 and '1' reload TLR2. Third 32 bit pattern

Definition at line 69 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_PATTERN4

Define the pattern, '0' relaod TLR1 and '1' reload TLR2. Fourth 32 bit pattern

Definition at line 72 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_PATTERN_SIZE

Define the pattern size to use. 7 bit pattern, 0x0 size of 1 and 0x7F size of 128

Definition at line 60 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_TLR1

Load TLR1 register. 32 bit value to load

Definition at line 54 of file BlueNRG1_rtc.h.

uint32_t RTC_InitType::RTC_TLR2

Load TLR2 register. 32 bit value to load

Definition at line 57 of file BlueNRG1_rtc.h.

The documentation for this struct was generated from the following file:

- BlueNRG1_rtc.h