| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
NVIC_InitType Struct Reference
BLUENRG1 Peripheral Driver » MISC Peripheral » Exported Types

Structure definition of NVIC initialization. More...

`#include <misc.h>`

## Public Attributes

uint8_t | NVIC_IRQChannel
uint8_t | NVIC_IRQChannelPreemptionPriority
FunctionalState | NVIC_IRQChannelCmd

## Detailed Description

Structure definition of NVIC initialization.

Definition at line 51 of file misc.h.

## Member Data Documentation

uint8_t NVIC_InitType::NVIC_IRQChannel

Specifies the IRQ channel to be enabled or disabled. This parameter can be a value of IRQn_Type (For the complete BlueNRG1 Device IRQ Channels list, please refer to BlueNRG1.h file)

Definition at line 53 of file misc.h.

FunctionalState NVIC_InitType::NVIC_IRQChannelCmd

Specifies whether the IRQ channel defined in NVIC_IRQChannel will be enabled or disabled. This parameter can be set either to ENABLE or DISABLE

Definition at line 62 of file misc.h.

uint8_t NVIC_InitType::NVIC_IRQChannelPreemptionPriority

Specifies the pre-emption priority for the IRQ channel specified in NVIC_IRQChannel. This parameter can be a value between 0 and 3

Definition at line 58 of file misc.h.

The documentation for this struct was generated from the following file:

- misc.h