| BlueNRG-1 Master/Central Library

- Main Page
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
devDiscoveryS Struct Reference

Device discovery parameters. More...

`#include <master_basic_profile.h>`

## Public Attributes

uint8_t | procedure
uint16_t | scanInterval
uint16_t | scanWindow
uint8_t | own_address_type

## Detailed Description

Device discovery parameters.

Definition at line 311 of file master_basic_profile.h.

## Member Data Documentation

uint8_t devDiscoveryS::own_address_type

Type of our address used during advertising (PUBLIC_ADDR, RANDOM_ADDR).

Definition at line 330 of file master_basic_profile.h.

uint8_t devDiscoveryS::procedure

Device discovery procedure used:

- LIMITED_DISCOVERY_PROCEDURE
- GENERAL_DISCOVERY_PROCEDURE

Definition at line 316 of file master_basic_profile.h.

uint16_t devDiscoveryS::scanInterval

Time interval from when the Controller started its last LE scan until it begins the subsequent LE scan. The scan interval should be a number in the range 0x0004 to 0x4000. This corresponds to a time range 2.5 msec to 10240 msec. For a number N, Time = N x 0.625 msec.

Definition at line 322 of file master_basic_profile.h.

uint16_t devDiscoveryS::scanWindow

Amount of time for the duration of the LE scan. The scan window shall be less than or equal to scan interval. The scan window should be a number in the range 0x0004 to 0x4000. This corresponds to a time range 2.5 msec to 10240 msec. For a number N, Time = N x 0.625 msec.

Definition at line 328 of file master_basic_profile.h.

The documentation for this struct was generated from the following file:

- master_basic_profile.h