| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Functions
Public Function
BLUENRG1 Peripheral Driver » MISC Peripheral

## Functions

void | NVIC_Init (NVIC_InitType *NVIC_InitStruct)
| Initializes the NVIC peripheral according to the specified parameters in the NVIC_InitStruct. More...
void | SystemSleepCmd (FunctionalState NewState)
| Enables or disables sleep/stop mode on system level. More...
void | SysTick_State (FunctionalState NewState)

## Detailed Description

## Function Documentation

void NVIC_Init | ( | NVIC_InitType * | NVIC_InitStruct | ) |

Initializes the NVIC peripheral according to the specified parameters in the NVIC_InitStruct.

Parameters

  NVIC_InitStruct | pointer to a NVIC_InitTypeDef structure that contains the configuration information for the specified NVIC peripheral.

Return values

  None |

Definition at line 87 of file misc.c.

void SystemSleepCmd | ( | FunctionalState | NewState | ) |

Enables or disables sleep/stop mode on system level.

Parameters

  NewState | functional state FunctionalState This parameter can be: ENABLE or DISABLE.

Return values

  None |

Enable Sleep/Stop mode entry on system level

Disable Sleep/Stop mode entry on system level

Definition at line 116 of file misc.c.

void SysTick_State | ( | FunctionalState | NewState | ) |

Definition at line 131 of file misc.c.