| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- i
- l
- s

### - i -

- i2c_buffer_rx : SDK_EVAL_I2C.c
- i2c_buffer_tx : SDK_EVAL_I2C.c
- i2c_eot : SDK_EVAL_I2C.c

### - l -

- LPS25HB_SlaveAddress : LPS25HB.c
- LPS25HBDrv : LPS25HB.h , LPS25HB.c
- LSM6DS3Drv : lsm6ds3.h
- LSM6DS3Drv_ext_internal : lsm6ds3.h

### - s -

- s_I2CBaseVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cClkPinModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_I2cClkPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataDmaRxTcVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_I2cDataDmaRxVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataDmaTxTcVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataDmaTxVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cDataModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_I2cDataPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_I2cPeripheralVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs1ModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs1PinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs2ModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiCs2PinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiIrqSensorPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiMisoModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_SpiMisoPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiMosiModeVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiMosiPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_SpiSclkModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_SpiSclkPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_UartRxModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_UartRxPinVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_UartTxModeVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_UartTxPinVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- s_vectnButtonPinVersion : USER_Platform_Configuration_auto.h , SDK_EVAL_Config.c
- s_vectnGpioPinVersion : SDK_EVAL_Config.c , USER_Platform_Configuration_auto.h
- spi_buffer_rx : SDK_EVAL_SPI.c
- spi_buffer_tx : SDK_EVAL_SPI.c
- spi_eot : SDK_EVAL_SPI.c