| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Delay Between Frames Definition
BLUENRG1 Peripheral Driver » SPI Peripheral » Exported Constants

## Macros

#define | IS_WAIT_VALUE(VALUE) ( (VALUE) < 16)

## Detailed Description

## Macro Definition Documentation

#define IS_WAIT_VALUE | ( |  | VALUE | ) | ( (VALUE) < 16)

Definition at line 298 of file BlueNRG1_spi.h.