| STM32L - BlueNRG-1 BLE stack APIs, Events and Constants

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
Bonded_Device_Entry_t_s Struct Reference

`#include <bluenrg1_gap_aci.h>`

## Public Attributes

uint8_t | Address_Type
uint8_t | Address [6]

## Detailed Description

Documentation for Bonded_Device_Entry_t

Definition at line 35 of file bluenrg1_gap_aci.h.

## Member Data Documentation

uint8_t Bonded_Device_Entry_t_s::Address[6]

Public Device Address or Random Device Address of the device to be added to the white list.

Definition at line 40 of file bluenrg1_gap_aci.h.

uint8_t Bonded_Device_Entry_t_s::Address_Type

0x00 Public Device Address 0x01 Random Device Address 0x02 - 0xFF Reserved for future use

Definition at line 38 of file bluenrg1_gap_aci.h.

The documentation for this struct was generated from the following file:

- bluenrg1_gap_aci.h