| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
LPS25HB_Output_Data_Rate_Selection_CTRL_REG1
SDK EVAL BlueNRG1 » LPS25HB » LPS25HB SENSOR LIB » LPS25HB_Exported_Defines

## Macros

#define | LPS25HB_ODR_ONE_SHOT ((uint8_t)0x00)
#define | LPS25HB_ODR_1Hz ((uint8_t)0x10)
#define | LPS25HB_ODR_7Hz ((uint8_t)0x20)
#define | LPS25HB_ODR_12_5Hz ((uint8_t)0x30)
#define | LPS25HB_ODR_25Hz ((uint8_t)0x40)
#define | LPS25HB_ODR_MASK ((uint8_t)0x70)

## Detailed Description

## Macro Definition Documentation

#define LPS25HB_ODR_12_5Hz ((uint8_t)0x30)

Output Data Rate: P - 12.5Hz, T - 12.5Hz

Definition at line 441 of file LPS25HB.h.

#define LPS25HB_ODR_1Hz ((uint8_t)0x10)

Output Data Rate: P - 1Hz, T - 1Hz

Definition at line 439 of file LPS25HB.h.

#define LPS25HB_ODR_25Hz ((uint8_t)0x40)

Output Data Rate: P - 25Hz, T - 25Hz

Definition at line 442 of file LPS25HB.h.

#define LPS25HB_ODR_7Hz ((uint8_t)0x20)

Output Data Rate: P - 7Hz, T - 7Hz

Definition at line 440 of file LPS25HB.h.

#define LPS25HB_ODR_MASK ((uint8_t)0x70)

Definition at line 444 of file LPS25HB.h.

#define LPS25HB_ODR_ONE_SHOT ((uint8_t)0x00)

Output Data Rate: P - one shot, T - one shot

Definition at line 438 of file LPS25HB.h.