| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Mic Frequency Definitions
BLUENRG1 Peripheral Driver » ADC Peripheral » Exported Constants

## Macros

#define | ADC_MIC_800KHZ ((uint8_t)0x00)
#define | ADC_MIC_1600KHZ ((uint8_t)0x01)
#define | IS_ADC_MIC_FREQ_SEL(FREQ) (((FREQ) == ADC_MIC_800KHZ) || ((FREQ) == ADC_MIC_1600KHZ))

## Detailed Description

## Macro Definition Documentation

#define ADC_MIC_1600KHZ ((uint8_t)0x01)

Enable the 1.6 MHz through IO0 for external MEMS microphone

Definition at line 173 of file BlueNRG1_adc.h.

#define ADC_MIC_800KHZ ((uint8_t)0x00)

Enable the 800 kHz through IO0 for external MEMS microphone

Definition at line 172 of file BlueNRG1_adc.h.

#define IS_ADC_MIC_FREQ_SEL | ( |  | FREQ | ) | (((FREQ) == ADC_MIC_800KHZ) || ((FREQ) == ADC_MIC_1600KHZ))

Definition at line 175 of file BlueNRG1_adc.h.