| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
SDK EVAL SPI Exported Constants
SDK EVAL BlueNRG1 » SDK EVAL SPI

## Macros

#define | SPI_BAUDRATE (1000000)
| SPI Baudrate. More...
#define | SPI_DR_BASE_ADDR (SPI_BASE + 0x08)
| SPI DR address. More...
#define | SPI_BUFF_SIZE (10)
| SPI buffer max size. More...
#define | DMA_CH_SPI_TX (DMA_CH5)
| SPI_TX DMA channel. More...
#define | DMA_CH_SPI_TX_IT_TC (DMA_FLAG_TC5)
| SPI_TX DMA Transfer Complete Interrupt. More...
#define | DMA_CH_SPI_RX (DMA_CH4)
| SPI_RX DMA channel. More...
#define | DMA_CH_SPI_RX_IT_TC (DMA_FLAG_TC4)
| SPI_RX DMA Transfer Complete Interrupt. More...

## Detailed Description

## Macro Definition Documentation

#define DMA_CH_SPI_RX (DMA_CH4)

SPI_RX DMA channel.

Definition at line 89 of file SDK_EVAL_SPI.h.

#define DMA_CH_SPI_RX_IT_TC (DMA_FLAG_TC4)

SPI_RX DMA Transfer Complete Interrupt.

Definition at line 94 of file SDK_EVAL_SPI.h.

#define DMA_CH_SPI_TX (DMA_CH5)

SPI_TX DMA channel.

Definition at line 79 of file SDK_EVAL_SPI.h.

#define DMA_CH_SPI_TX_IT_TC (DMA_FLAG_TC5)

SPI_TX DMA Transfer Complete Interrupt.

Definition at line 84 of file SDK_EVAL_SPI.h.

#define SPI_BAUDRATE (1000000)

SPI Baudrate.

Definition at line 64 of file SDK_EVAL_SPI.h.

#define SPI_BUFF_SIZE (10)

SPI buffer max size.

Definition at line 74 of file SDK_EVAL_SPI.h.

#define SPI_DR_BASE_ADDR (SPI_BASE + 0x08)

SPI DR address.

Definition at line 69 of file SDK_EVAL_SPI.h.