| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
LPS25HB_Interrupt_Circuit_Enable_CTRL_REG1
SDK EVAL BlueNRG1 » LPS25HB » LPS25HB SENSOR LIB » LPS25HB_Exported_Defines

## Macros

#define | LPS25HB_DIFF_DISABLE ((uint8_t)0x00)
#define | LPS25HB_DIFF_ENABLE ((uint8_t)0x08)
#define | LPS25HB_DIFF_EN_MASK ((uint8_t)0x08)

## Detailed Description

## Macro Definition Documentation

#define LPS25HB_DIFF_DISABLE ((uint8_t)0x00)

interrupt circuit enabled

Definition at line 452 of file LPS25HB.h.

#define LPS25HB_DIFF_EN_MASK ((uint8_t)0x08)

Definition at line 455 of file LPS25HB.h.

#define LPS25HB_DIFF_ENABLE ((uint8_t)0x08)

interrupt generation disabled

Definition at line 453 of file LPS25HB.h.