| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
PWMX Pins Definitions
BLUENRG1 Peripheral Driver » MFT Peripheral » Exported Constants

## Macros

#define | MFT_PWM0_PIN GPIO_Pin_2 /* The PWM0 pin */
#define | MFT_PWM1_PIN GPIO_Pin_3 /* The PWM1 pin */
#define | IS_MFT_PWMX_PIN(VALUE) (((VALUE) == MFT_PWM0_PIN) || ((VALUE) == MFT_PWM1_PIN))

## Detailed Description

## Macro Definition Documentation

#define IS_MFT_PWMX_PIN | ( |  | VALUE | ) | (((VALUE) == MFT_PWM0_PIN) || ((VALUE) == MFT_PWM1_PIN))

Definition at line 190 of file BlueNRG1_mft.h.

#define MFT_PWM0_PIN GPIO_Pin_2 /* The PWM0 pin */

Definition at line 187 of file BlueNRG1_mft.h.

#define MFT_PWM1_PIN GPIO_Pin_3 /* The PWM1 pin */

Definition at line 188 of file BlueNRG1_mft.h.