| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
LSM6DS3_XG_FIFO_Mode_Selection_FIFO_CTRL5
SDK EVAL BlueNRG1 » LSM6DS3 » LSM6DS3 SENSOR LIB » LSM6DS3_Exported_Defines

## Macros

#define | LSM6DS3_XG_FIFO_MODE_BYPASS ((uint8_t)0x00)
#define | LSM6DS3_XG_FIFO_MODE_FIFO ((uint8_t)0x01)
#define | LSM6DS3_XG_FIFO_MODE_CONTINUOUS_THEN_FIFO ((uint8_t)0x03)
#define | LSM6DS3_XG_FIFO_MODE_BYPASS_THEN_CONTINUOUS ((uint8_t)0x04)
#define | LSM6DS3_XG_FIFO_MODE_CONTINUOUS_OVERWRITE ((uint8_t)0x05)
#define | LSM6DS3_XG_FIFO_MODE_MASK ((uint8_t)0x07)

## Detailed Description

## Macro Definition Documentation

#define LSM6DS3_XG_FIFO_MODE_BYPASS ((uint8_t)0x00)

BYPASS Mode. FIFO turned off

Definition at line 1054 of file lsm6ds3.h.

#define LSM6DS3_XG_FIFO_MODE_BYPASS_THEN_CONTINUOUS ((uint8_t)0x04)

BYPASS mode until trigger is deasserted, then CONTINUOUS mode

Definition at line 1057 of file lsm6ds3.h.

#define LSM6DS3_XG_FIFO_MODE_CONTINUOUS_OVERWRITE ((uint8_t)0x05)

CONTINUOUS mode. If the FIFO is full the new sample overwrite the older one

Definition at line 1058 of file lsm6ds3.h.

#define LSM6DS3_XG_FIFO_MODE_CONTINUOUS_THEN_FIFO ((uint8_t)0x03)

CONTINUOUS mode until trigger is deasserted, then FIFO mode

Definition at line 1056 of file lsm6ds3.h.

#define LSM6DS3_XG_FIFO_MODE_FIFO ((uint8_t)0x01)

FIFO Mode. Stop collecting data when FIFO is full

Definition at line 1055 of file lsm6ds3.h.

#define LSM6DS3_XG_FIFO_MODE_MASK ((uint8_t)0x07)

Definition at line 1060 of file lsm6ds3.h.