| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Exported Types
BLUENRG1 Peripheral Driver » FLASH Peripheral

## Macros

#define | Flash_CMDDONE 0x01 /* Flash command done */
| Flash status enumeration. More...
#define | Flash_CMDSTART 0x02 /* Flash command start */
#define | Flash_CMDERR 0x04 /* Flash command error */
#define | Flash_ILLCMD 0x08 /* Flash illegal command written */
#define | Flash_READOK 0x10 /* Flash mass read was OK */
#define | Flash_FLNREADY 0x20 /* Flash not ready (sleep) */
#define | IS_FLASH_FLAG(FLAG)

## Detailed Description

## Macro Definition Documentation

#define Flash_CMDDONE 0x01 /* Flash command done */

Flash status enumeration.

Definition at line 50 of file BlueNRG1_flash.h.

#define Flash_CMDERR 0x04 /* Flash command error */

Definition at line 52 of file BlueNRG1_flash.h.

#define Flash_CMDSTART 0x02 /* Flash command start */

Definition at line 51 of file BlueNRG1_flash.h.

#define Flash_FLNREADY 0x20 /* Flash not ready (sleep) */

Definition at line 55 of file BlueNRG1_flash.h.

#define Flash_ILLCMD 0x08 /* Flash illegal command written */

Definition at line 53 of file BlueNRG1_flash.h.

#define Flash_READOK 0x10 /* Flash mass read was OK */

Definition at line 54 of file BlueNRG1_flash.h.

#define IS_FLASH_FLAG | ( |  | FLAG | ) |

Value:
( ((FLAG) == Flash_CMDDONE) || \
((FLAG) == Flash_CMDSTART) || \
((FLAG) == Flash_CMDERR) || \
((FLAG) == Flash_ILLCMD) || \
((FLAG) == Flash_READOK) || \
((FLAG) == Flash_FLNREADY) )
Flash_CMDSTART
#define Flash_CMDSTART
Definition: BlueNRG1_flash.h:51
Flash_READOK
#define Flash_READOK
Definition: BlueNRG1_flash.h:54
Flash_FLNREADY
#define Flash_FLNREADY
Definition: BlueNRG1_flash.h:55
Flash_CMDDONE
#define Flash_CMDDONE
Flash status enumeration.
Definition: BlueNRG1_flash.h:50
Flash_CMDERR
#define Flash_CMDERR
Definition: BlueNRG1_flash.h:52
Flash_ILLCMD
#define Flash_ILLCMD
Definition: BlueNRG1_flash.h:53

Definition at line 57 of file BlueNRG1_flash.h.