| BlueNRG-1 HAL drivers APIs

- Main Page
- Classes
- Files

- File List
- File Members

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- f
- g
- h
- i
- l
- n
- o
- p
- r
- s
- t
- w

### - a -

- APP_HIGHER_ADDRESS : OTA_btl.h
- APP_HIGHER_ADDRESS_END : OTA_btl.h
- APP_LOWER_ADDRESS : OTA_btl.h
- APP_LOWER_ADDRESS_END : OTA_btl.h
- APP_OTA_SERVICE_ADDRESS : OTA_btl.h
- APP_WITH_OTA_SERVICE_ADDRESS : OTA_btl.h
- APP_WITH_OTA_SERVICE_PAGE_NUMBER_END : OTA_btl.h
- APP_WITH_OTA_SERVICE_PAGE_NUMBER_START : OTA_btl.h
- ASSERT_HANDLER : crash_handler.h
- ASSERT_SIGNATURE : crash_handler.h

### - b -

- BLUENRG_SLEEP_CONFIGURATION_ERROR : sleep.h

### - c -

- CRASH_HANDLER : crash_handler.h
- CRASH_INFO_BASE_ADDRESS : crash_handler.h
- CRASH_RAM_SIZE : crash_handler.h

### - f -

- FALSE : hal_types.h
- FLASH_PAGE_SIZE : OTA_btl.h

### - g -

- GET_CRASH_INFO : crash_handler.h

### - h -

- HARD_FAULT_SIGNATURE : crash_handler.h
- HIGHER_APPLICATION_BASE_OFFSET : OTA_btl.h
- HOST_TO_LE_16 : hal_types.h
- HOST_TO_LE_32 : hal_types.h

### - i -

- IS_ERROR_STATE : hal_types.h
- IS_FLAGSTATUS : hal_types.h
- IS_FUNCTIONAL_STATE : hal_types.h
- IS_ITSTATUS : hal_types.h

### - l -

- LE_TO_HOST_32 : hal_types.h

### - n -

- NMB_OF_EXCEP_RAM_WORD : crash_handler.h
- NMI_SIGNATURE : crash_handler.h
- NO_WAKEUP_RESET : sleep.h

### - o -

- OTA_APP_SWITCH_OP_CODE_GO_TO_HIGHER_APP : OTA_btl.h
- OTA_APP_SWITCH_OP_CODE_GO_TO_LOWER_APP : OTA_btl.h
- OTA_APP_SWITCH_OP_CODE_GO_TO_NEW_APP : OTA_btl.h
- OTA_APP_SWITCH_OP_CODE_GO_TO_OTA_SERVICE_MANAGER : OTA_btl.h
- OTA_APP_SWITCH_OP_CODE_NO_OPERATION : OTA_btl.h
- OTA_BASIC_APPLICATION_BASE_OFFSET : OTA_btl.h
- OTA_HIGHER_APPLICATION_PAGE_NUMBER_END : OTA_btl.h
- OTA_HIGHER_APPLICATION_PAGE_NUMBER_START : OTA_btl.h
- OTA_IN_PROGRESS_TAG : OTA_btl.h
- OTA_INVALID_OLD_TAG : OTA_btl.h
- OTA_LOWER_APPLICATION_PAGE_NUMBER_END : OTA_btl.h
- OTA_LOWER_APPLICATION_PAGE_NUMBER_START : OTA_btl.h
- OTA_LOWER_HIGHER_APPLICATION_AVAILABLE_SECTORS_NUMBERS : OTA_btl.h
- OTA_NO_OPERATION : OTA_btl.h
- OTA_RESET_MANAGER_PAGE_NUMBER_START : OTA_btl.h
- OTA_RESET_MANAGER_PAGE_NUMBERS : OTA_btl.h
- OTA_SERVICE_MANAGER_RAM_LOCATION : OTA_btl.h
- OTA_SERVICE_MANAGER_TAG : OTA_btl.h
- OTA_SET_SERVICE_MANAGER_RAM_LOCATION : OTA_btl.h
- OTA_TAG_VECTOR_TABLE_ENTRY_INDEX : OTA_btl.h
- OTA_TAG_VECTOR_TABLE_ENTRY_OFFSET : OTA_btl.h
- OTA_VALID_TAG : OTA_btl.h

### - p -

- PRINTF : OTA_btl.h

### - r -

- RESET_MANAGER_FLASH_BASE_ADDRESS : OTA_btl.h
- RESET_MANAGER_FLASH_BASE_OFFSET : OTA_btl.h

### - s -

- SLEEP_TIMER : sleep.h

### - t -

- TRUE : hal_types.h

### - w -

- WAKEUP_BOR : sleep.h
- WAKEUP_IO10 : sleep.h
- WAKEUP_IO11 : sleep.h
- WAKEUP_IO12 : sleep.h
- WAKEUP_IO13 : sleep.h
- WAKEUP_IO9 : sleep.h
- WAKEUP_IO_HIGH : sleep.h
- WAKEUP_IO_LOW : sleep.h
- WAKEUP_POR : sleep.h
- WAKEUP_RESET_WDG : sleep.h
- WAKEUP_SLEEP_TIMER1 : sleep.h
- WAKEUP_SLEEP_TIMER2 : sleep.h
- WAKEUP_SYS_RESET_REQ : sleep.h
- WATCHDOG_SIGNATURE : crash_handler.h