| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
SDK EVAL LPS25HB_HAL Exported Functions
SDK EVAL BlueNRG1 » LPS25HB » SDK EVAL LPS25HB_HAL

## Macros

#define | LPS25HB_I2C_FREQUENCY (10000)
#define | LPS25HB_IO_Init() (PRESSURE_StatusTypeDef)SdkEvalI2CInit(LPS25HB_I2C_FREQUENCY)
#define | LPS25HB_IO_Write(pBuffer, DeviceAddr, RegisterAddr, NumByteToWrite) (PRESSURE_StatusTypeDef)SdkEvalI2CWrite(pBuffer, DeviceAddr, RegisterAddr, NumByteToWrite)
#define | LPS25HB_IO_Read(pBuffer, DeviceAddr, RegisterAddr, NumByteToRead) (PRESSURE_StatusTypeDef)SdkEvalI2CRead(pBuffer, DeviceAddr, RegisterAddr, NumByteToRead)
#define | LPS25HB_IO_ITConfig()

## Detailed Description

## Macro Definition Documentation

#define LPS25HB_I2C_FREQUENCY (10000)

Definition at line 80 of file LPS25HB_hal.h.

#define LPS25HB_IO_Init | ( |  | void | ) | (PRESSURE_StatusTypeDef)SdkEvalI2CInit(LPS25HB_I2C_FREQUENCY)

Definition at line 98 of file LPS25HB_hal.h.

#define LPS25HB_IO_ITConfig | ( |  | void | ) |

Definition at line 105 of file LPS25HB_hal.h.

#define LPS25HB_IO_Read | ( |  | pBuffer,
|  |  | DeviceAddr,
|  |  | RegisterAddr,
|  |  | NumByteToRead
| ) |  | (PRESSURE_StatusTypeDef)SdkEvalI2CRead(pBuffer, DeviceAddr, RegisterAddr, NumByteToRead)

Definition at line 100 of file LPS25HB_hal.h.

#define LPS25HB_IO_Write | ( |  | pBuffer,
|  |  | DeviceAddr,
|  |  | RegisterAddr,
|  |  | NumByteToWrite
| ) |  | (PRESSURE_StatusTypeDef)SdkEvalI2CWrite(pBuffer, DeviceAddr, RegisterAddr, NumByteToWrite)

Definition at line 99 of file LPS25HB_hal.h.