| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Hold Time
BLUENRG1 Peripheral Driver » I2C Peripheral » Exported Constants

## Macros

#define | IS_I2C_HOLDTIME(TIME) ((TIME) <= 0x1FF)

## Detailed Description

## Macro Definition Documentation

#define IS_I2C_HOLDTIME | ( |  | TIME | ) | ((TIME) <= 0x1FF)

This macro checks if the hold time is a valid value

Definition at line 325 of file BlueNRG1_i2c.h.