| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
LSM6DS3_XG_Accelerometer_Anti_Aliasing_Filter_Bandwidth_Selection_CTRL1_XL
SDK EVAL BlueNRG1 » LSM6DS3 » LSM6DS3 SENSOR LIB » LSM6DS3_Exported_Defines

## Macros

#define | LSM6DS3_XL_BW_400HZ ((uint8_t)0x00)
#define | LSM6DS3_XL_BW_200HZ ((uint8_t)0x01)
#define | LSM6DS3_XL_BW_100HZ ((uint8_t)0x02)
#define | LSM6DS3_XL_BW_50HZ ((uint8_t)0x03)
#define | LSM6DS3_XL_BW_MASK ((uint8_t)0x03)

## Detailed Description

## Macro Definition Documentation

#define LSM6DS3_XL_BW_100HZ ((uint8_t)0x02)

Anti-aliasing filter bandwidht: 100 Hz

Definition at line 1192 of file lsm6ds3.h.

#define LSM6DS3_XL_BW_200HZ ((uint8_t)0x01)

Anti-aliasing filter bandwidht: 200 Hz

Definition at line 1191 of file lsm6ds3.h.

#define LSM6DS3_XL_BW_400HZ ((uint8_t)0x00)

Anti-aliasing filter bandwidht: 400 Hz

Definition at line 1190 of file lsm6ds3.h.

#define LSM6DS3_XL_BW_50HZ ((uint8_t)0x03)

Anti-aliasing filter bandwidht: 50 Hz

Definition at line 1193 of file lsm6ds3.h.

#define LSM6DS3_XL_BW_MASK ((uint8_t)0x03)

Definition at line 1195 of file lsm6ds3.h.