| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Peripheral Incremented Mode Definitions
BLUENRG1 Peripheral Driver » DMA Peripheral » Exported Constants

## Macros

#define | DMA_PeripheralInc_Enable ((uint32_t)0x00000040)
#define | DMA_PeripheralInc_Disable ((uint32_t)0x00000000)
#define | IS_DMA_PERIPHERAL_INC_STATE(STATE)

## Detailed Description

## Macro Definition Documentation

#define DMA_PeripheralInc_Disable ((uint32_t)0x00000000)

Definition at line 112 of file BlueNRG1_dma.h.

#define DMA_PeripheralInc_Enable ((uint32_t)0x00000040)

Definition at line 111 of file BlueNRG1_dma.h.

#define IS_DMA_PERIPHERAL_INC_STATE | ( |  | STATE | ) |

Value:
(((STATE) == DMA_PeripheralInc_Enable) || \
((STATE) == DMA_PeripheralInc_Disable))
DMA_PeripheralInc_Enable
#define DMA_PeripheralInc_Enable
Definition: BlueNRG1_dma.h:111
DMA_PeripheralInc_Disable
#define DMA_PeripheralInc_Disable
Definition: BlueNRG1_dma.h:112

Definition at line 113 of file BlueNRG1_dma.h.