| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Variables
SDK EVAL Config Public Variables
SDK EVAL BlueNRG1 » SDK EVAL Config

## Variables

const uint32_t | s_vectnButtonPinVersion [SDK_PLATFORMS_NUMBER][EVAL_BOARD_BUTTONS] = {{GPIO_Pin_13, GPIO_Pin_5}}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) Buttons definitions. More...
const uint32_t | s_UartTxPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_8}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) UART definitions. More...
const uint32_t | s_UartTxModeVersion [SDK_PLATFORMS_NUMBER] = {Serial1_Mode}
const uint32_t | s_UartRxPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_11}
const uint32_t | s_UartRxModeVersion [SDK_PLATFORMS_NUMBER] = {Serial1_Mode}
const I2C_Type * | s_I2cPeripheralVersion [SDK_PLATFORMS_NUMBER] = {I2C2}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) I2C definitions. More...
const uint32_t | s_I2cDataPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_5}
const uint32_t | s_I2cDataModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_I2cClkPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_4}
const uint32_t | s_I2cClkPinModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const DMA_CH_Type * | s_I2cDataDmaTxVersion [SDK_PLATFORMS_NUMBER] = {DMA_CH7}
const uint32_t | s_I2cDataDmaRxTcVersion [SDK_PLATFORMS_NUMBER] = {DMA_FLAG_TC6}
const DMA_CH_Type * | s_I2cDataDmaRxVersion [SDK_PLATFORMS_NUMBER] = {DMA_CH6}
const uint32_t | s_I2cDataDmaTxTcVersion [SDK_PLATFORMS_NUMBER] = {DMA_FLAG_TC7}
const uint32_t | s_I2CBaseVersion [SDK_PLATFORMS_NUMBER] = {I2C2_BASE}
const uint32_t | s_vectnGpioPinVersion [SDK_PLATFORMS_NUMBER][EVAL_BOARD_LEDS] = {{GPIO_Pin_6, GPIO_Pin_7, GPIO_Pin_14}}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) LEDs definitions. More...
const uint32_t | s_SpiCs1PinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_1}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) SPI definitions. More...
const uint32_t | s_SpiCs1ModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiCs2PinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_11}
const uint32_t | s_SpiCs2ModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiMosiPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_2}
const uint32_t | s_SpiMosiModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiMisoPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_3}
const uint32_t | s_SpiMisoModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiSclkPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_0}
const uint32_t | s_SpiSclkModeVersion [SDK_PLATFORMS_NUMBER] = {Serial0_Mode}
const uint32_t | s_SpiIrqSensorPinVersion [SDK_PLATFORMS_NUMBER] = {GPIO_Pin_12}
| BlueNRG1 Eval Board (STEVAL-IDB007V1) sensor IRQ definitions. More...

## Detailed Description

## Variable Documentation

const uint32_t s_I2CBaseVersion[SDK_PLATFORMS_NUMBER] = {I2C2_BASE}

Definition at line 102 of file SDK_EVAL_Config.c.

const uint32_t s_I2cClkPinModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 94 of file SDK_EVAL_Config.c.

const uint32_t s_I2cClkPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_4}

Definition at line 93 of file SDK_EVAL_Config.c.

const uint32_t s_I2cDataDmaRxTcVersion[SDK_PLATFORMS_NUMBER] = {DMA_FLAG_TC6}

Definition at line 97 of file SDK_EVAL_Config.c.

const DMA_CH_Type* s_I2cDataDmaRxVersion[SDK_PLATFORMS_NUMBER] = {DMA_CH6}

Definition at line 99 of file SDK_EVAL_Config.c.

const uint32_t s_I2cDataDmaTxTcVersion[SDK_PLATFORMS_NUMBER] = {DMA_FLAG_TC7}

Definition at line 100 of file SDK_EVAL_Config.c.

const DMA_CH_Type* s_I2cDataDmaTxVersion[SDK_PLATFORMS_NUMBER] = {DMA_CH7}

Definition at line 96 of file SDK_EVAL_Config.c.

const uint32_t s_I2cDataModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 92 of file SDK_EVAL_Config.c.

const uint32_t s_I2cDataPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_5}

Definition at line 91 of file SDK_EVAL_Config.c.

const I2C_Type* s_I2cPeripheralVersion[SDK_PLATFORMS_NUMBER] = {I2C2}

BlueNRG1 Eval Board (STEVAL-IDB007V1) I2C definitions.

BlueNRG1 Eval Board (STEVAL-IDB007VX) I2C definitions.

Definition at line 90 of file SDK_EVAL_Config.c.

const uint32_t s_SpiCs1ModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 115 of file SDK_EVAL_Config.c.

const uint32_t s_SpiCs1PinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_1}

BlueNRG1 Eval Board (STEVAL-IDB007V1) SPI definitions.

BlueNRG1 Eval Board (STEVAL-IDB007VX) SPI definitions.

Definition at line 114 of file SDK_EVAL_Config.c.

const uint32_t s_SpiCs2ModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 117 of file SDK_EVAL_Config.c.

const uint32_t s_SpiCs2PinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_11}

Definition at line 116 of file SDK_EVAL_Config.c.

const uint32_t s_SpiIrqSensorPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_12}

BlueNRG1 Eval Board (STEVAL-IDB007V1) sensor IRQ definitions.

Definition at line 128 of file SDK_EVAL_Config.c.

const uint32_t s_SpiMisoModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 121 of file SDK_EVAL_Config.c.

const uint32_t s_SpiMisoPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_3}

Definition at line 120 of file SDK_EVAL_Config.c.

const uint32_t s_SpiMosiModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 119 of file SDK_EVAL_Config.c.

const uint32_t s_SpiMosiPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_2}

Definition at line 118 of file SDK_EVAL_Config.c.

const uint32_t s_SpiSclkModeVersion[SDK_PLATFORMS_NUMBER] = {Serial0_Mode}

Definition at line 123 of file SDK_EVAL_Config.c.

const uint32_t s_SpiSclkPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_0}

Definition at line 122 of file SDK_EVAL_Config.c.

const uint32_t s_UartRxModeVersion[SDK_PLATFORMS_NUMBER] = {Serial1_Mode}

Definition at line 84 of file SDK_EVAL_Config.c.

const uint32_t s_UartRxPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_11}

Definition at line 83 of file SDK_EVAL_Config.c.

const uint32_t s_UartTxModeVersion[SDK_PLATFORMS_NUMBER] = {Serial1_Mode}

Definition at line 82 of file SDK_EVAL_Config.c.

const uint32_t s_UartTxPinVersion[SDK_PLATFORMS_NUMBER] = {GPIO_Pin_8}

BlueNRG1 Eval Board (STEVAL-IDB007V1) UART definitions.

BlueNRG1 Eval Board (STEVAL-IDB007VX) UART definitions.

Definition at line 81 of file SDK_EVAL_Config.c.

const uint32_t s_vectnButtonPinVersion[SDK_PLATFORMS_NUMBER][EVAL_BOARD_BUTTONS] = {{GPIO_Pin_13, GPIO_Pin_5}}

BlueNRG1 Eval Board (STEVAL-IDB007V1) Buttons definitions.

BlueNRG1 Eval Board (STEVAL-IDB007VX) Buttons definitions.

Definition at line 75 of file SDK_EVAL_Config.c.

const uint32_t s_vectnGpioPinVersion[SDK_PLATFORMS_NUMBER][EVAL_BOARD_LEDS] = {{GPIO_Pin_6, GPIO_Pin_7, GPIO_Pin_14}}

BlueNRG1 Eval Board (STEVAL-IDB007V1) LEDs definitions.

BlueNRG1 Eval Board (STEVAL-IDB007VX) LEDs definitions.

Definition at line 107 of file SDK_EVAL_Config.c.