| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Mode1a Trigger Definitions
BLUENRG1 Peripheral Driver » MFT Peripheral » Exported Constants

## Macros

#define | MFT_TnB_TRIGGER ((uint32_t)0x0) /* trigger on TnB edge */
#define | MFT_SOFTWARE_TRIGGER ((uint32_t)0x1) /* trigger software */
#define | IS_MFT_PULSETRAIN_TRIGGER(MODE) (((MODE) == MFT_TnB_TRIGGER) || ((MODE) == MFT_SOFTWARE_TRIGGER))

## Detailed Description

## Macro Definition Documentation

#define IS_MFT_PULSETRAIN_TRIGGER | ( |  | MODE | ) | (((MODE) == MFT_TnB_TRIGGER) || ((MODE) == MFT_SOFTWARE_TRIGGER))

Definition at line 164 of file BlueNRG1_mft.h.

#define MFT_SOFTWARE_TRIGGER ((uint32_t)0x1) /* trigger software */

Definition at line 162 of file BlueNRG1_mft.h.

#define MFT_TnB_TRIGGER ((uint32_t)0x0) /* trigger on TnB edge */

Definition at line 161 of file BlueNRG1_mft.h.