| STM32L - BlueNRG-1 BLE stack APIs, Events and Constants

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
Advertising_Report_t_s Struct Reference
HCI LE meta events

`#include <bluenrg1_events.h>`

## Public Attributes

uint8_t | Event_Type
uint8_t | Address_Type
uint8_t | Address [6]
uint8_t | Length_Data
uint8_t * | Data
uint8_t | RSSI

## Detailed Description

Documentation for Advertising_Report_t

Definition at line 191 of file bluenrg1_events.h.

## Member Data Documentation

uint8_t Advertising_Report_t_s::Address[6]

Public Device Address or Random Device Address of the device to be connected

Definition at line 202 of file bluenrg1_events.h.

uint8_t Advertising_Report_t_s::Address_Type

0x00 Public Device Address 0x01 Random Device Address 0x02 - 0xFF Reserved for future use

Definition at line 200 of file bluenrg1_events.h.

uint8_t* Advertising_Report_t_s::Data

Length_Data[i] octets of advertising or scan response data formatted as defined in [Vol 3] Part C, Section 8.

Definition at line 206 of file bluenrg1_events.h.

uint8_t Advertising_Report_t_s::Event_Type

0x00 Connectable undirected advertising (ADV_IND). 0x01 Connectable directed advertising (ADV_DIRECT_IND) 0x02 Scannable undirected advertising (ADV_SCAN_IND) 0x03 Non connectable undirected advertising (ADV_NONCONN_IND) 0x04 Scan Response (SCAN_RSP) 0x05-0xFF Reserved for future use

Definition at line 197 of file bluenrg1_events.h.

uint8_t Advertising_Report_t_s::Length_Data

0x00 - 0x1F Length of the Data[i] field for each device which responded. 0x20 - 0xFF Reserved for future use.

Definition at line 204 of file bluenrg1_events.h.

uint8_t Advertising_Report_t_s::RSSI

N Size: 1 Octet (signed integer) Range: -127 <= N <= +20 Units: dBm 127 RSSI is not available 21 to 126 Reserved for future use

Definition at line 211 of file bluenrg1_events.h.

The documentation for this struct was generated from the following file:

- bluenrg1_events.h