| BlueNRG-1 ACI APIs and events callbacks

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

Macros
hci_const.h File Reference

This file defines constants and functions for HCI layer. More...

Go to the source code of this file.

## Macros

#define | HCI_UNKNOWN_COMMAND 0x01
#define | HCI_NO_CONNECTION 0x02
#define | HCI_HARDWARE_FAILURE 0x03
#define | HCI_PAGE_TIMEOUT 0x04
#define | HCI_AUTHENTICATION_FAILURE 0x05
#define | HCI_PIN_OR_KEY_MISSING 0x06
#define | HCI_MEMORY_FULL 0x07
#define | HCI_CONNECTION_TIMEOUT 0x08
#define | HCI_MAX_NUMBER_OF_CONNECTIONS 0x09
#define | HCI_MAX_NUMBER_OF_SCO_CONNECTIONS 0x0a
#define | HCI_ACL_CONNECTION_EXISTS 0x0b
#define | HCI_COMMAND_DISALLOWED 0x0c
#define | HCI_REJECTED_LIMITED_RESOURCES 0x0d
#define | HCI_REJECTED_SECURITY 0x0e
#define | HCI_REJECTED_PERSONAL 0x0f
#define | HCI_HOST_TIMEOUT 0x10
#define | HCI_UNSUPPORTED_FEATURE 0x11
#define | HCI_INVALID_PARAMETERS 0x12
#define | HCI_OE_USER_ENDED_CONNECTION 0x13
#define | HCI_OE_LOW_RESOURCES 0x14
#define | HCI_OE_POWER_OFF 0x15
#define | HCI_CONNECTION_TERMINATED 0x16
#define | HCI_REPEATED_ATTEMPTS 0x17
#define | HCI_PAIRING_NOT_ALLOWED 0x18
#define | HCI_UNKNOWN_LMP_PDU 0x19
#define | HCI_UNSUPPORTED_REMOTE_FEATURE 0x1a
#define | HCI_SCO_OFFSET_REJECTED 0x1b
#define | HCI_SCO_INTERVAL_REJECTED 0x1c
#define | HCI_AIR_MODE_REJECTED 0x1d
#define | HCI_INVALID_LMP_PARAMETERS 0x1e
#define | HCI_UNSPECIFIED_ERROR 0x1f
#define | HCI_UNSUPPORTED_LMP_PARAMETER_VALUE 0x20
#define | HCI_ROLE_CHANGE_NOT_ALLOWED 0x21
#define | HCI_LMP_RESPONSE_TIMEOUT 0x22
#define | HCI_LMP_ERROR_TRANSACTION_COLLISION 0x23
#define | HCI_LMP_PDU_NOT_ALLOWED 0x24
#define | HCI_ENCRYPTION_MODE_NOT_ACCEPTED 0x25
#define | HCI_UNIT_LINK_KEY_USED 0x26
#define | HCI_QOS_NOT_SUPPORTED 0x27
#define | HCI_INSTANT_PASSED 0x28
#define | HCI_PAIRING_NOT_SUPPORTED 0x29
#define | HCI_TRANSACTION_COLLISION 0x2a
#define | HCI_QOS_UNACCEPTABLE_PARAMETER 0x2c
#define | HCI_QOS_REJECTED 0x2d
#define | HCI_CLASSIFICATION_NOT_SUPPORTED 0x2e
#define | HCI_INSUFFICIENT_SECURITY 0x2f
#define | HCI_PARAMETER_OUT_OF_RANGE 0x30
#define | HCI_ROLE_SWITCH_PENDING 0x32
#define | HCI_SLOT_VIOLATION 0x34
#define | HCI_ROLE_SWITCH_FAILED 0x35
#define | HCI_EIR_TOO_LARGE 0x36
#define | HCI_SIMPLE_PAIRING_NOT_SUPPORTED 0x37
#define | HCI_HOST_BUSY_PAIRING 0x38
#define | HCI_CONN_REJ_NO_CH_FOUND 0x39
#define | HCI_CONTROLLER_BUSY 0x3A
#define | HCI_UNACCEPTABLE_CONN_INTERV 0x3B
#define | HCI_DIRECTED_ADV_TIMEOUT 0x3C
#define | HCI_CONN_TERM_MIC_FAIL 0x3D
#define | HCI_CONN_FAIL_TO_BE_ESTABL 0x3E
#define | HCI_MAC_CONN_FAILED 0x3F

## Detailed Description

This file defines constants and functions for HCI layer.

Author
  AMS - VMA RF Application team

Version
  V1.0.0

Date
  21-Sept-2015

Attention

THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.

##
© COPYRIGHT 2015 STMicroelectronics

Definition in file hci_const.h.