| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Timer Operating Mode Definitions
BLUENRG1 Peripheral Driver » RTC Peripheral » Exported Constants

## Macros

#define | RTC_TIMER_PERIODIC ((uint8_t)0)
#define | RTC_TIMER_ONESHOT ((uint8_t)1)
#define | IS_RTC_TIMER_MODE(IT)

## Detailed Description

## Macro Definition Documentation

#define IS_RTC_TIMER_MODE | ( |  | IT | ) |

Value:
(((IT) == RTC_TIMER_PERIODIC) || \
((IT) == RTC_TIMER_ONESHOT))
RTC_TIMER_PERIODIC
#define RTC_TIMER_PERIODIC
Definition: BlueNRG1_rtc.h:177
RTC_TIMER_ONESHOT
#define RTC_TIMER_ONESHOT
Definition: BlueNRG1_rtc.h:178

This macro checks if IT is a valid combination of interrupt

Definition at line 182 of file BlueNRG1_rtc.h.

#define RTC_TIMER_ONESHOT ((uint8_t)1)

RTC timer one shot mode

Definition at line 178 of file BlueNRG1_rtc.h.

#define RTC_TIMER_PERIODIC ((uint8_t)0)

RTC timer periodic mode

Definition at line 177 of file BlueNRG1_rtc.h.