| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
FIFO Level Definition
BLUENRG1 Peripheral Driver » UART Peripheral » Exported Constants

## Macros

#define | FIFO_LEV_1_8 ((uint8_t)0)
#define | FIFO_LEV_1_4 ((uint8_t)1)
#define | FIFO_LEV_1_2 ((uint8_t)2)
#define | FIFO_LEV_3_4 ((uint8_t)3)
#define | FIFO_LEV_7_8 ((uint8_t)4)
#define | IS_FIFO_LEV(FIFO_LEV)

## Detailed Description

## Macro Definition Documentation

#define FIFO_LEV_1_2 ((uint8_t)2)

Interrupt FIFO becomes >= 1/2 full

Definition at line 231 of file BlueNRG1_uart.h.

#define FIFO_LEV_1_4 ((uint8_t)1)

Interrupt FIFO becomes >= 1/4 full

Definition at line 230 of file BlueNRG1_uart.h.

#define FIFO_LEV_1_8 ((uint8_t)0)

Interrupt FIFO becomes >= 1/8 full

Definition at line 229 of file BlueNRG1_uart.h.

#define FIFO_LEV_3_4 ((uint8_t)3)

Interrupt FIFO becomes >= 3/4 full

Definition at line 232 of file BlueNRG1_uart.h.

#define FIFO_LEV_7_8 ((uint8_t)4)

Interrupt FIFO becomes >= 7/8 full

Definition at line 233 of file BlueNRG1_uart.h.

#define IS_FIFO_LEV | ( |  | FIFO_LEV | ) |

Value:
( ((FIFO_LEV) == FIFO_LEV_1_8) || \
((FIFO_LEV) == FIFO_LEV_1_4) || \
((FIFO_LEV) == FIFO_LEV_1_2) || \
((FIFO_LEV) == FIFO_LEV_3_4) || \
((FIFO_LEV) == FIFO_LEV_7_8))
FIFO_LEV_1_4
#define FIFO_LEV_1_4
Definition: BlueNRG1_uart.h:230
FIFO_LEV_1_8
#define FIFO_LEV_1_8
Definition: BlueNRG1_uart.h:229
FIFO_LEV_3_4
#define FIFO_LEV_3_4
Definition: BlueNRG1_uart.h:232
FIFO_LEV_1_2
#define FIFO_LEV_1_2
Definition: BlueNRG1_uart.h:231
FIFO_LEV_7_8
#define FIFO_LEV_7_8
Definition: BlueNRG1_uart.h:233

Definition at line 236 of file BlueNRG1_uart.h.