| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Members

Public Attributes | List of all members
MFT_InitType Struct Reference
BLUENRG1 Peripheral Driver » MFT Peripheral » Exported Types

Structure definition of MFT initialization. More...

`#include <BlueNRG1_mft.h>`

## Public Attributes

uint8_t | MFT_Mode
uint8_t | MFT_Clock1
uint8_t | MFT_Clock2
uint8_t | MFT_Prescaler
uint16_t | MFT_CRA
uint16_t | MFT_CRB

## Detailed Description

Structure definition of MFT initialization.

Definition at line 49 of file BlueNRG1_mft.h.

## Member Data Documentation

uint8_t MFT_InitType::MFT_Clock1

Specifies the MFT clock selection, for counter A. This value can be a value of MFT_Clock_Selector_Definition

Definition at line 54 of file BlueNRG1_mft.h.

uint8_t MFT_InitType::MFT_Clock2

Specifies the MFT clock selection, for counter B. This value can be a value of MFT_Clock_Selector_Definition

Definition at line 57 of file BlueNRG1_mft.h.

uint16_t MFT_InitType::MFT_CRA

Specifies the MFT CRA init value.

Definition at line 62 of file BlueNRG1_mft.h.

uint16_t MFT_InitType::MFT_CRB

Specifies the MFT CRB init value.

Definition at line 64 of file BlueNRG1_mft.h.

uint8_t MFT_InitType::MFT_Mode

Specifies the MFT mode. This value can be a value of MFT_Mode_Definition

Definition at line 51 of file BlueNRG1_mft.h.

uint8_t MFT_InitType::MFT_Prescaler

Specifies the MFT prescaler.

Definition at line 60 of file BlueNRG1_mft.h.

The documentation for this struct was generated from the following file:

- BlueNRG1_mft.h