| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

Variables
SDK EVAL SPI Private Variable
SDK EVAL BlueNRG1 » SDK EVAL SPI

## Variables

volatile uint8_t | spi_buffer_tx [SPI_BUFF_SIZE]
| SPI buffers used for DMA application. More...
volatile uint8_t | spi_buffer_rx [SPI_BUFF_SIZE]
volatile FlagStatus | spi_eot = SET
| SPI flag set at end of transaction. More...

## Detailed Description

## Variable Documentation

volatile uint8_t spi_buffer_rx[SPI_BUFF_SIZE]

Definition at line 74 of file SDK_EVAL_SPI.c.

volatile uint8_t spi_buffer_tx[SPI_BUFF_SIZE]

SPI buffers used for DMA application.

Definition at line 73 of file SDK_EVAL_SPI.c.

volatile FlagStatus spi_eot = SET

SPI flag set at end of transaction.

Definition at line 79 of file SDK_EVAL_SPI.c.