| BlueNRG-1 SDK drivers APIs

- Main Page
- Modules
- Classes
- Files

- File List
- File Members

Macros
USER_Platform_Configuration.h File Reference

This file contains definitions for BlueNRG-1 Eval Platform. More...

`#include "BlueNRG1.h"`
`#include "BlueNRG1_conf.h"`

Go to the source code of this file.

## Macros

#define | PUSH_BUTTON1_PIN GPIO_Pin_13
| BlueNRG1 Eval Board (STEVAL-IDB007Vx) Buttons definitions. More...
#define | PUSH_BUTTON2_PIN GPIO_Pin_5
#define | SDK_EVAL_UART_TX_PIN GPIO_Pin_8
| BlueNRG1 Eval Board (STEVAL-IDB007Vx) UART definitions. More...
#define | SDK_EVAL_UART_TX_MODE Serial1_Mode
#define | SDK_EVAL_UART_RX_PIN GPIO_Pin_11
#define | SDK_EVAL_UART_RX_MODE Serial1_Mode
#define | SDK_EVAL_I2C I2C2
| BlueNRG1 Eval Board (STEVAL-IDB007Vx) I2C definitions. More...
#define | SDK_EVAL_I2C_DATA_PIN GPIO_Pin_5
#define | SDK_EVAL_I2C_DATA_MODE Serial0_Mode
#define | SDK_EVAL_I2C_CLK_PIN GPIO_Pin_4
#define | SDK_EVAL_I2C_CLK_MODE Serial0_Mode
#define | SDK_EVAL_I2C_IRQ_HANDLER I2C2_Handler
#define | SDK_EVAL_I2C_DMA_TX DMA_CH7
#define | SDK_EVAL_I2C_DMA_TX_ITTC DMA_FLAG_TC7
#define | SDK_EVAL_I2C_DMA_RX DMA_CH6
#define | SDK_EVAL_I2C_DMA_RX_ITTC DMA_FLAG_TC6
#define | SDK_EVAL_I2C_BASE I2C2_BASE
#define | SDK_EVAL_LED1_PIN GPIO_Pin_6
| BlueNRG1 Eval Board (STEVAL-IDB007Vx) LEDs definitions. More...
#define | SDK_EVAL_LED2_PIN GPIO_Pin_7
#define | SDK_EVAL_LED3_PIN GPIO_Pin_14
#define | SDK_EVAL_SPI_PERIPH_SENSOR_PIN GPIO_Pin_1
| BlueNRG1 Eval Board (STEVAL-IDB007Vx) SPI definitions. More...
#define | SDK_EVAL_SPI_PERIPH_SENSOR_MODE Serial0_Mode
#define | SDK_EVAL_SPI_PERIPH_MOSI_PIN GPIO_Pin_2
#define | SDK_EVAL_SPI_PERIPH_MOSI_MODE Serial0_Mode
#define | SDK_EVAL_SPI_PERIPH_MISO_PIN GPIO_Pin_3
#define | SDK_EVAL_SPI_PERIPH_MISO_MODE Serial0_Mode
#define | SDK_EVAL_SPI_PERIPH_SCLK_PIN GPIO_Pin_0
#define | SDK_EVAL_SPI_PERIPH_SCLK_MODE Serial0_Mode
#define | SDK_EVAL_IRQ_SENSOR_PIN GPIO_Pin_12

## Detailed Description

This file contains definitions for BlueNRG-1 Eval Platform.

Author
  AMS VMA RF application team

Version
  V1.0.0

Date
  September 29, 2015 THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.

THIS SOURCE CODE IS PROTECTED BY A LICENSE. FOR MORE INFORMATION PLEASE CAREFULLY READ THE LICENSE AGREEMENT FILE LOCATED IN THE ROOT DIRECTORY OF THIS FIRMWARE PACKAGE.

##
© COPYRIGHT 2015 STMicroelectronics

Definition in file USER_Platform_Configuration.h.

## Macro Definition Documentation

#define PUSH_BUTTON1_PIN GPIO_Pin_13

BlueNRG1 Eval Board (STEVAL-IDB007Vx) Buttons definitions.

Definition at line 39 of file USER_Platform_Configuration.h.

#define PUSH_BUTTON2_PIN GPIO_Pin_5

Definition at line 40 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C I2C2

BlueNRG1 Eval Board (STEVAL-IDB007Vx) I2C definitions.

Definition at line 56 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_BASE I2C2_BASE

Definition at line 72 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_CLK_MODE Serial0_Mode

Definition at line 62 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_CLK_PIN GPIO_Pin_4

Definition at line 61 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_DATA_MODE Serial0_Mode

Definition at line 59 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_DATA_PIN GPIO_Pin_5

Definition at line 58 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_DMA_RX DMA_CH6

Definition at line 69 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_DMA_RX_ITTC DMA_FLAG_TC6

Definition at line 70 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_DMA_TX DMA_CH7

Definition at line 66 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_DMA_TX_ITTC DMA_FLAG_TC7

Definition at line 67 of file USER_Platform_Configuration.h.

#define SDK_EVAL_I2C_IRQ_HANDLER I2C2_Handler

Definition at line 64 of file USER_Platform_Configuration.h.

#define SDK_EVAL_IRQ_SENSOR_PIN GPIO_Pin_12

Definition at line 99 of file USER_Platform_Configuration.h.

#define SDK_EVAL_LED1_PIN GPIO_Pin_6

BlueNRG1 Eval Board (STEVAL-IDB007Vx) LEDs definitions.

Definition at line 78 of file USER_Platform_Configuration.h.

#define SDK_EVAL_LED2_PIN GPIO_Pin_7

Definition at line 79 of file USER_Platform_Configuration.h.

#define SDK_EVAL_LED3_PIN GPIO_Pin_14

Definition at line 80 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_MISO_MODE Serial0_Mode

Definition at line 94 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_MISO_PIN GPIO_Pin_3

Definition at line 93 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_MOSI_MODE Serial0_Mode

Definition at line 91 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_MOSI_PIN GPIO_Pin_2

Definition at line 90 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_SCLK_MODE Serial0_Mode

Definition at line 97 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_SCLK_PIN GPIO_Pin_0

Definition at line 96 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_SENSOR_MODE Serial0_Mode

Definition at line 88 of file USER_Platform_Configuration.h.

#define SDK_EVAL_SPI_PERIPH_SENSOR_PIN GPIO_Pin_1

BlueNRG1 Eval Board (STEVAL-IDB007Vx) SPI definitions.

Definition at line 87 of file USER_Platform_Configuration.h.

#define SDK_EVAL_UART_RX_MODE Serial1_Mode

Definition at line 50 of file USER_Platform_Configuration.h.

#define SDK_EVAL_UART_RX_PIN GPIO_Pin_11

Definition at line 49 of file USER_Platform_Configuration.h.

#define SDK_EVAL_UART_TX_MODE Serial1_Mode

Definition at line 47 of file USER_Platform_Configuration.h.

#define SDK_EVAL_UART_TX_PIN GPIO_Pin_8

BlueNRG1 Eval Board (STEVAL-IDB007Vx) UART definitions.

Definition at line 46 of file USER_Platform_Configuration.h.