| BlueNRG-1 Peripherals drivers APIs

- Main Page
- Modules
- Classes
- Files

Macros
Clock Speed
BLUENRG1 Peripheral Driver » I2C Peripheral » Exported Constants

## Macros

#define | IS_I2C_CLOCK_SPEED_I2C(SPEED) (((SPEED) >= 1) && ((SPEED) <= 400000))

## Detailed Description

## Macro Definition Documentation

#define IS_I2C_CLOCK_SPEED_I2C | ( |  | SPEED | ) | (((SPEED) >= 1) && ((SPEED) <= 400000))

This macro checks if I2C baud rate is a valid value

Definition at line 290 of file BlueNRG1_i2c.h.